- Top
- Overview
- What you can do with this camera
- Connecting to the network

# Connecting to the network

## Wired LAN connection

The following operations are available on your computer via LAN terminal:

- Camera status check

- Thumbnail image check

- Proxy playback

- Download of proxy file/clip management information

- Displaying/editing of metadata

- Adding/deleting of metadata (shot mark or text memo)

- Camera remote control (collective operations of recording control and time code/user bits)

In addition, the following operations are available via the LAN terminal.

- Transferring of clips with the FTP client function

- Remote control function using the Remote Operation Panel (AK-HRP200G)

## Connection using wireless LAN and 4G/LTE

Attaching the wireless module AJ-WM30 (optional) to the <USB2.0 HOST> terminal (sub-host) of the camera allows you to connect the camera via wireless LAN (IEEE 802.11).

The following operations are available using your tablet, smartphone, and computer.

- Camera status check

- Thumbnail image check

- Proxy playback

- Displaying/editing of metadata

- Adding/deleting of metadata (shot mark or text memo)

- Camera remote control (collective operations of recording control and time code/user bits)

In addition, clips can be transferred by the FTP client function via wireless LAN (access point connection) or 4G/LTE.

Top of the page