- Top
- Preparation
- Assigning functions to the USER buttons
- Selectable functions

# Selectable functions

Item | Description
--- | ---
[INHIBIT] | Disables assignment of functions.
[SCENE FILE SEL] | Assigns the function to display the screen (the main menu → [SCENE FILE] → [FILE SELECT]) in which users select the scene file.
[LEVEL GAUGE] | Switches the level gauge display function to enabled/disabled.
[LEVEL GAUGE RESET] | Assigns the function to set the level gauge using the current horizontal and vertical directions as reference values. Holding down the assigned button will reset to the factory setting.
[WFM] | Assigns the function for switching the waveform display. Select the waveform display from the main menu → [SW MODE] → [WFM MODE].
[D.ZOOM] | Assigns the digital zoom function. Zooms in on the field angle by 2x, 5x, and 10x vertically and horizontally.
[DRS] | Assigns the dynamic range stretcher function.
[FBC] | Switches the flash band compensation function to enabled/disabled.
[S.GAIN] | Assigns the function that increases the gain to 24 dB or more. Select the gain value from the main menu → [SW MODE] → [SUPER GAIN].
[1S.EXP.] | Enables/disables the one second exposure function.
[ATW] | Switches the auto tracking white balance functions to enabled/disabled.
[ATW LOCK] | Fixes the white balance value when pressing this item while the auto tracking white balance function is activated. Resumes the auto tracking white balance function when pressing again.
[SPOTLIGHT] | Switches the auto iris control function for the spot light to enabled/disabled.
[BACKLIGHT] | Switches the auto iris control function for the backlight compensation to enabled/disabled.
[BLACKFADE] | Assigns the functions that fade out the entire image as black.
[WHITEFADE] | Assigns the functions that fade out the entire image as white.
[A.IRIS LEVEL] | Switches the auto iris setting function to enabled/disabled.
[IRIS] | Assigns the function for switching the auto iris and manual iris.
[Y GET] | Assigns the function for displaying the luminance level of the image at the position indicated by the square marker displayed near the center.
[FOCUS ASSIST] | Enables/disables the focus assist function which is set in the main menu → [SW MODE] → [FOCUS ASSIST MODE].
[FOCUS MACRO] | Switches the macro focus setting. You can set the macro function effects in the main menu → [SW MODE] → [MACRO MODE].
[OIS] | Switches the image stabilizer to enabled/disabled.
[FAST ZOOM] | Speeds up the zoom speed when the zoom lever (with the HANDLE ZOOM switch at the handle side set to <VAR>) is pushed in to the end.
[ZEBRA] | Assigns the display function of the zebra pattern and marker.
[EVF ON/OFF] | Assigns the function that forces images to be displayed in the viewfinder.
[PRE REC] | Assigns the function for switching the pre-recording function to enabled/disabled.
[TEXT MEMO] | Assigns the text memo function.
[SHOT MARK] | Assigns the shot mark function.
[DEL LAST CLIP] | Assigns the function to delete the clip shot immediately beforehand.
[SLOT SEL] | Assigns the function for switching the card to record when two or more cards are inserted in the microP2 memory card slot.
[REC MEDIA] | Assigns the function to select the recording target slot between the P2 memory card slot and microP2 memory card slot. This setting is linked to the setting value in the main menu → [RECORDING SETUP] → [REC MEDIA].
[AUDIO MON SEL] | Assigns the function that switches between the display of the audio level meter and the audio channel ([CH1]/[CH2] and [CH3]/[CH4]) of output audio (headphones, built-in speaker, <AUDIO OUT> terminal, and <HDMI OUT> terminal) while the button is held down.
[REC CHECK] | Assigns the recording check function.
[BACKGR REC PAUSE] | Assigns the function to cancel the background recording of slot 2. Hold down the assigned button for approx. five seconds to stop the background recording.
[USB MODE] | Assigns the function for switching the USB device mode or USB host mode to enabled/disabled.
[PLAYLIST] | Assigns the function for switching entering/exiting of the playlist edit mode.
[REC DURING UPLOAD] | Assigns the function for enabling/disabling the rec during upload function. This setting is linked to the setting value in the main menu → [NETWORK SETUP] → [FTP CLIENT SERVICE] → [REC DURING UPLOAD].
[UPLOAD LIST] | Assigns the function to display the upload list of the rec during upload function. To close the upload list, press the <EXIT> button.
[STREAMING START] | Assigns the function for starting/stopping streaming from the camera. This setting is linked to the setting value in the main menu → [NETWORK SETUP] → [STREAMING SETTING] → [START].
[LOAD USER FILE] | Assigns the function to display the selection screen for the user file saved on the SD memory card. This does not function in the thumbnail screen.

NOTE

- The following functions are also turned off when the camera is turned off.

  [WFM]/[D.ZOOM]/[FBC]/[S.GAIN]/[ATW]/[ATW LOCK]/[SPOTLIGHT]/[BACKLIGHT]/[BLACKFADE]/[WHITEFADE]/[Y GET]/[FOCUS ASSIST]/[FAST ZOOM]/[EVF ON/OFF]/[AUDIO MON SEL]/[USB MODE]/[PLAYLIST]

- When [FAST ZOOM] is enabled, the zoom sound becomes louder than usual.

Top of the page