- Top
- Shooting
- Dual codec recording

# Dual codec recording

Recording in different formats for main recording and sub recording can be performed on the camera.

For sub recording, you can select HD proxy in AVC-LongG 6 format with 1920×1080 resolution or one of three SD proxies with different resolution.

The file format is MOV that is suitable for nonlinear editing.

For the combination with the main recording, refer to “System modes and recording functions”.

Dual codec recording setting
Recording the proxy data
Recording to the SD memory card
Checking the proxy data
Error displays about proxy data recordings
Top of the page