- Top
- Preparation
- Tally lamp

# Tally lamp

If set to anything other than [OFF] in the main menu → [OTHER FUNCTIONS] → [TALLY LAMP], you can make up the tally lamp light while photographing.

Also, the tally lamp will flash when the following situations occur:

- The P2 card has less free space to record and the battery level is low (one time per second)

- The P2 card has been removed while being accessed (four times per second)

- The P2 card has no more space to record (four times per second)

- When the warnings such as the fluctuation of the reference signal for the <GENLOCK IN/VIDEO OUT> terminal and a system error or recording abnormality warning are displayed (four times per second)

Front tally lamp

Rear tally lamp

Top of the page