- Top
- Shooting
- Selecting audio input and adjusting recording levels
- Selecting audio input signals

# Selecting audio input signals

Select the audio signal to be recorded to audio channel 1/2.

Audio channel 3/4 is automatically determined by the <CH1 SELECT> and <CH2 SELECT> settings.

<CH1 SELECT> switch | Subjects recorded on channel 1 | Subjects recorded on channel 3
--- | --- | ---
<INT(L)> | L audio of built-in microphone | Microphone and device connected to <AUDIO INPUT 1>
<INPUT1> | Microphone and device connected to <AUDIO INPUT 1> | L audio of built-in microphone
<INPUT2> | Microphone and device connected to <AUDIO INPUT 2> | L audio of built-in microphone

<CH2 SELECT> switch | Subjects recorded on channel 2 | Subjects recorded on channel 4
--- | --- | ---
<INT(R)> | R audio of built-in microphone | Microphone and device connected to <AUDIO INPUT 2>
<INPUT1> | Microphone and device connected to <AUDIO INPUT 1> | R audio of built-in microphone
<INPUT2> | Microphone and device connected to <AUDIO INPUT 2> | R audio of built-in microphone

You can set the number of audio bits recorded in accordance with the format.

For details, refer to “System modes and recording functions”.

Format | Number of audio bits
--- | ---
[AVC-I100] [AVC-I50] | You can select [24BIT] and [16BIT]. You can select the main menu → [SYSTEM MODE] → [AUDIO SMPL RES].
[AVC-I200] [AVC-G50] [AVC-G25] | [24BIT] fixed.
[AVC-G12] [DVCPRO HD] [DVCPRO50] [DVCPRO] [DV] | [16BIT] fixed.

Top of the page