- Top
- Menu Operations
- Setting menu display
- Setting menu basic operations

# Setting menu basic operations

You can change camera settings using the setting menu according to the shooting scene and recording details.

The menu is divided into the main menu, submenu, and setting item menu.

Set data are written and saved in the internal memory of the camera.

Menu items can be selected by control stick operation or the <SEL/PUSH SET> dial button operation.

This section describes main menu operations. Main menu operation is the same as the other menus except when opening the menu screen.

1. <EXIT> button

2. Control stick

3. <MENU> button (Operation panel of the LCD monitor)

4. <SHIFT> button

5. <SEL/PUSH SET> dial button

6. <MENU> button

7. <MODE/MENU CANCEL> button

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Fig. 5

#### Selecting menu item using control stick

Press and hold the <MENU> button for three seconds or more when not recording.

- The main menu screen is displayed in the viewfinder and on the LCD monitor.

Press the control stick upward/downward to place the cursor on the desired menu item. (Fig. 1)

- The cursor moves up/down by pushing the control stick upward/downward.

- If there is a menu in the next level, [] is displayed in the menu items.

  Pressing the control stick to the right or pressing the control stick opens the lower-level menus. (Fig. 2)

- Pressing the control stick to the left or pressing the <EXIT> button returns the upper level of menu.

Press the control stick.

- The confirmation screen is displayed depending on the menu item.

  Press the control stick upward/downward/to the left/to the right to select the operation, and then press the control stick.

  A checkmark is placed in front of the set item.

- In some menus, a screen for setting value is displayed on the menu screen (Fig. 3) or at the bottom of the screen (Fig. 4).

- In some menus, a message is displayed if a menu cannot be executed.

Press the <MENU> button to close the menu.

- This brings you back automatically to the previous screen depending on the menu item.

#### Selecting menu item with the <SEL/PUSH SET> dial button

Press and hold the <MENU> button for three seconds or more when not recording.

- The main menu screen is displayed in the viewfinder and on the LCD monitor.

Turn the <SEL/PUSH SET> dial button to place the cursor on the desired menu item. (Fig. 1)

- The cursor moves up/down by turning the <SEL/PUSH SET> dial button upward/downward.

- If there is a menu in the next level, [] is displayed in the menu items.

  Pressing the <SEL/PUSH SET> dial button opens the lower-level menus. (Fig. 2)

- You can go back to the upper levels by pressing the <EXIT> button or by placing the cursor on the topmost line ([EXIT]) then pressing the <SEL/PUSH SET> dial button.

Press the <SEL/PUSH SET> dial button.

- The confirmation screen is displayed depending on the menu item.

  Turn the <SEL/PUSH SET> dial button to select the operation, and then press the <SEL/PUSH SET> dial button.

  A checkmark is placed in front of the set item.

- In some menus, a screen for setting value is displayed on the menu screen (Fig. 3) or at the bottom of the screen (Fig. 4).

- In some menus, a message is displayed if a menu cannot be executed.

Press the <MENU> button to close the menu.

- This brings you back automatically to the previous screen depending on the menu item.

#### Performing cancellation while setting

Press the <MODE/MENU CANCEL> button. Alternatively, press the <EXIT> button while holding down the <SHIFT> button.

[MENU CANCEL BACK TO PREV] is displayed. (Fig. 5)

Press the <MODE/MENU CANCEL> button again. Alternatively, press the <EXIT> button while holding down the <SHIFT> button.

The changed value returns to the value before changing.

NOTE

- A restart of the camera is required when the system frequency setting or the number of lines, or the network connection method is changed.

Top of the page