- Top
- Specification
- Specifications
- Specifications

# Specifications

## General

Power DC 7.2 V (when the battery is used) DC 12 V (when the AC adaptor is used) Power consumption 19.5 W (when the LCD monitor is used)

indicates safety information.

Ambient operating temperature | 0 °C - 40 °C (32 °F - 104 °F)
Ambient operating humidity | 10% - 80% (no condensation)
Weight | Approx. 2.2 kg (4.9 lbs.) (body only, excluding lens hood, battery, and accessories) Approx. 2.6 kg (5.7 lbs.) (including lens hood, supplied battery, and microphone holder)
Dimensions (W×H×D) | Body only 176 mm×171 mm×329 mm (6-15/16 inches×6-23/32 inches×12-15/16 inches) (excluding protrusion)

## Camera unit

Pickup device | 1/3-type 2.2 million pixels, MOS solid state image sensor ×3
Lens | Optical image stabilizer lens, optical 22x motorized zoom F1.6 - F3.2 (f=3.9 mm - 86 mm) 35 mm conversion: 28 mm - 616 mm (16:9)
Filter diameter | 72 mm
Color separation optical system | Prism system
ND filter | <OFF>, <1/4>, <1/16>, <1/64>
Shortest shooting distance (M.O.D) | 1.1 m from the lens
Gain setting | <L>/<M>/<H> selector switch −3 dB – 18 dB (in 1 dB steps) (Negative value of gain is only in [HIGH SENS.] mode.) (When assigning [S.GAIN] to the USER button: Switching between 24 dB, 30 dB, and 36 dB)
Color temperature setting | [ATW], [ATW LOCK], [Ach], [Bch], preset 3200 K/preset 5600 K/VAR (2000 K to 15000 K)
Shutter speed | When [SYSTEM MODE] = 59.94 Hz 60i/60p mode: 1/60 (shutter off), 1/100, 1/120, 1/250, 1/500, 1/1000, 1/2000 sec. 30p mode: 1/30, 1/50 (shutter off), 1/60, 1/120, 1/250, 1/500, 1/1000, 1/2000 sec. 24p mode: 1/24, 1/50 (shutter off), 1/60, 1/120, 1/250, 1/500, 1/1000, 1/2000 sec.
When [SYSTEM MODE] = 50 Hz 50i/50p mode: 1/50 (shutter off), 1/60, 1/120, 1/250, 1/500, 1/1000, 1/2000 sec. 25p mode: 1/25, 1/50 (shutter off), 1/60, 1/120, 1/250, 1/500, 1/1000, 1/2000 sec.
Slow shutter speed | Setting is possible when [VFR]=[OFF] When [SYSTEM MODE] = 59.94 Hz 60i/60p mode: 1/1, 1/2, 1/4, 1/6, 1/15, 1/30 sec. 30p mode: 1/1, 1/2, 1/4, 1/6, 1/15 sec. 24p mode: 1/1, 1/2, 1/4, 1/6, 1/12 sec.
When [SYSTEM MODE] = 50 Hz 50i/50p mode: 1/1, 1/2, 1/4, 1/6, 1/12, 1/25 sec. 25p mode: 1/1, 1/2, 1/4, 1/6, 1/12 sec.
Synchro scan shutter | When [SYSTEM MODE] = 59.94 Hz and [SYNC SCAN TYPE] = [sec] 60i/60p mode: 1/60.0 – 1/249.8 sec. 30p mode: 1/30.0 – 1/249.8 sec. 24p mode: 1/24.0 – 1/249.8 sec.
When [SYSTEM MODE] = 50 Hz and [SYNC SCAN TYPE] = [sec] 50i/50p mode: 1/50.0 – 1/250.0 sec. 25p mode: 1/25.0 – 1/250.0 sec.
Shutter open angle | 3.0 deg – 180.0 deg – 360.0 deg (in 0.5 deg steps, angle display)
VFR recording frame rate | 1080/59.94p: 1, 2, 4, 6, 9, 12, 15, 18, 20, 21, 22, 24, 25, 26, 27, 28, 30, 32, 34, 36, 40, 44, 48, 54, and 60 (frames per second) 1080/50p: 1, 2, 4, 6, 9, 12, 15, 18, 20, 21, 22, 23, 24, 25, 26, 27, 28, 30, 32, 34, 37, 42, 45, 48, and 50 (frames per second)
Sensitivity | [HIGH SENS.] mode F11 (2000 lx, 3200 K, 89.9% reflection, 1080/59.94i) F12 (2000 lx, 3200 K, 89.9% reflection, 1080/50i)
Minimum subject illumination | 0.02 lx (F1.6, gain 18 dB, [1S.EXP.], [HIGH SENS.] mode)
Digital zoom | x2/x5/x10
Lens hood | Hood with lens cover

## Memory card recorder

Recording media | microP2 memory card, P2 memory card
Recording slot | microP2 memory card slot ×2, P2 memory card slot ×1
System format | 1080/59.94p, 1080/59.94i, 1080/23.98PsF, 720/59.94p, 480/59.94i 1080/50p, 1080/50i, 720/50p, 576/50i
Recording format | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50 AVC-LongG 50/AVC-LongG 25/AVC-LongG 12 Switching DVCPRO HD/DVCPRO50/DVCPRO/DV formats
Recording video signal | 1080/59.94p, 1080/59.94i, 1080/29.97pN, 1080/23.98pN 720/59.94p, 720/29.97pN, 720/23.98pN 480/59.94i, 480/29.97p 1080/50p, 1080/50i, 1080/25pN 720/50p, 720/25pN 576/50i, 576/25p
Recording and playback time | AVC-Intra 200 16 GB×1 approx. 8 min 32 GB×1 approx. 16 min 64 GB×1 approx. 32 min AVC-Intra 100/DVCPRO HD 16 GB×1 approx. 16 min 32 GB×1 approx. 32 min 64 GB×1 approx. 64 min AVC-Intra 50/AVC-LongG 50/DVCPRO50 16 GB×1 approx. 32 min 32 GB×1 approx. 64 min 64 GB×1 approx. 128 min AVC-LongG 25/DVCPRO/DV 16 GB×1 approx. 64 min 32 GB×1 approx. 128 min 64 GB×1 approx. 256 min AVC-LongG 12 16 GB×1 approx. 120 min 32 GB×1 approx. 240 min 64 GB×1 approx. 480 min
Figures are for continuous recording as one clip. Depending on the number of clips, the overall recording time may be shorter than the above.

## Digital video

Sampling frequency | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50/AVC-LongG 50/AVC-LongG 25/AVC-LongG 12/DVCPRO HD Y: 74.1758 MHz, PB/PR: 37.0879 MHz (59.94 Hz) Y: 74.2500 MHz, PB/PR: 37.1250 MHz (50 Hz) DVCPRO50 Y: 13.5 MHz, PB/PR: 6.75 MHz DVCPRO Y: 13.5 MHz, PB/PR: 3.375 MHz
Quantizing | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50/AVC-LongG 50/AVC-LongG 25: 10 bits AVC-LongG 12/DVCPRO HD/DVCPRO50/DVCPRO/DV: 8 bits
Video compression format | AVC-Intra 200/AVC-Intra 100/AVC-Intra 50: MPEG-4 AVC/H.264 Intra Profile AVC-LongG 50/AVC-LongG 25/AVC-LongG 12: MPEG-4 AVC/H.264 DVCPRO HD: DV-Based Compression (SMPTE 370M) DVCPRO50/DVCPRO: DV-Based Compression (SMPTE 314M) DV: DV Compression (IEC 61834-2)

## Digital audio

Recording audio signal | AVC-Intra 200 48 kHz/24 bits, 4CH AVC-Intra 100/ AVC-Intra 50: 48 kHz/16 bits, 4CH and 48 kHz/24 bits, 4CH switch AVC-LongG 50/AVC-LongG 25: 48 kHz/24 bits, 4CH AVC-LongG 12/DVCPRO HD/DVCPRO50: 48 kHz/16 bits, 4CH DVCPRO/DV: 48 kHz/16 bits, 4CH
Headroom | 12 dB/18 dB/20 dB switchable menu

## AVC proxy

File format | MOV
Video compression format | H.264/AVC Baseline Profile H.264/AVC High Profile
Audio compression format | AAC-LC Linear PCM
Approximate recording time (1 GB) | AVC-G6 2CH MOV: Approx. 13 min SHQ 2CH MOV: Approx. 25 min HQ 2CH MOV: Approx. 78 min LOW 2CH MOV: Approx. 135 min
These are reference values for continuous recording using the Panasonic products. The recording time may differ depending on the scene or the number of clips.

## Video input/output

<SDI OUT> terminal | BNC×1
HD (3G/1.5G), SD: 0.8 V [p-p], 75 Ω
<VIDEO OUT> terminal | BNC×1
Also used as the <GENLOCK IN> terminal, <IN/OUT> switch selection
Composite: 1.0 V [p-p], 75 Ω
<HDMI OUT> terminal | HDMI×1 (HDMI type A terminal, not compatible with VIERA Link)

## Audio input

Built-in microphone | Supports stereo microphone
<AUDIO INPUT 1>/<AUDIO INPUT 2> terminal | XLR×2, 3-pin Input high impedance, <LINE>/<MIC> switch selection <LINE>: 4/0 dBu (selectable menu) <MIC>: −40/−50/−60 dBu (selectable menu), <+48V> on/off (switch selection)

## Audio output

<AUDIO OUT> terminal | 3.5 mm diameter stereo mini jack ×1 Output level: 600 Ω, 316 mV
Headphones terminal | 3.5 mm diameter stereo mini jack ×1 100 Ω, −16 dBV (32 Ω load, at maximum output level)
Speaker | 20 mm diameter, round ×1

## Other input/output

<CAM REMOTE> terminal | 2.5 mm diameter super mini jack ×1 <ZOOM S/S> 3.5 mm diameter mini jack ×1 <FOCUS IRIS>
<GENLOCK IN> terminal | BNC×1, also used as the <VIDEO OUT> terminal, <IN/OUT> switch selection, 1.0 V [p-p], 75 Ω
<TC IN/OUT> terminal | BNC×1 Used as the input and output terminals, <IN/OUT> switch selection Input: 1.0 V - 4.0 V [p-p], 10 kΩ Output: 2.0 V ± 0.5 V [p-p], low impedance
<LAN> terminal | 100BASE-TX/10BASE-T
<USB2.0 DEVICE> terminal (device) | Type miniB connector, 4-pin
<USB3.0 HOST> terminal (host) | Type A connector, 9-pin
<USB2.0 HOST> terminal (sub-host) | Type A connector, 4-pin (for the wireless module)
<DC IN 12V> terminal | DC 12 V (DC 10.5 V - 13.5 V), EIAJ type 4

## Monitor

LCD monitor | 3.5-type QHD color monitor (Approx. 1560000 dots)
Viewfinder | 0.5-type OLED (organic EL display) (Approx. 2360000 dots, video display area: approx. 1770000 dots)

## AC adaptor

Power source AC 100 V - 240 V, 50 Hz/60 Hz, 1.2 A Power output DC 12 V, 3.0 A

indicates safety information.

Ambient operating temperature | 0 °C - 40 °C (32 °F - 104 °F)
Ambient operating humidity | 10% - 80% (no condensation)
Weight | Approx. 210 g (0.46 lbs.)
Dimensions (W×H×D) | 115 mm×37 mm×57 mm (4-17/32 inches×1-15/32 inches×2-1/4 inches)

## Battery charger

Power source AC 100 V - 240 V, 50 Hz/60 Hz 0.4 A Power output DC 8.4 V, 1.2 A

indicates safety information.

Ambient operating temperature | 0 °C - 40 °C (32 °F - 104 °F)
Ambient operating humidity | 10% - 80% (no condensation)
Weight | Approx. 160 g (0.35 lbs.)
Dimensions (W×H×D) | 70 mm×44.5 mm×116 mm (2-3/4 inches×1-3/4 inches×4-9/16 inches)

Top of the page