- Top
- Shooting
- Adjustable settings when shooting
- Area mode function

# Area mode function

You can perform the following operations by displaying the area frame with the control stick.

- Area auto focus function

  Auto focus operation is performed within the area selected with the area frame.

- Area auto iris function

  The iris value is adjusted automatically within the area selected with the area frame.

- Area brightness display

  The luminance level of the center of the selected area frame is displayed.

## Operation function settings

Set the operations to be assigned to the area mode function from the main menu.

Select the desired function in the main menu → [SW MODE] → [AREA MODE].

- [INHIBIT]: Does not assign a function.

- [FOCUS]: Area focus function and area focus bar function (When [FOCUS BAR] is set)

- [IRIS]: Area iris function

- [Y GET]: Area brightness display

- [FOCUS/IRIS]: Simultaneous operation of area focus function/area iris function, and area focus bar function (When [FOCUS BAR] is set)

- [FOCUS/Y GET]: Simultaneous operation of area focus function/area brightness display, and area focus bar function (When [FOCUS BAR] is set)

## Operation of area mode function

The function set in the main menu → [SW MODE] → [AREA MODE] can be used by performing the following operation when shooting or while in shooting standby.

Press the control stick.

- An area frame (white) is displayed.

Press the control stick upward/downward/to the left/to the right to move the area frame to a desired position.

Press the control stick.

- The area frame color changes from white to yellow.

- When the yellow frame is displayed, the function set for [AREA MODE] can be operated in the area frame.

- While the function is activated, [AREA] is displayed on the right of the display.

- When the area brightness display is activated, the brightness display in the center does not operate.

Press the control stick for two seconds or longer.

- The area frame disappears and the camera exits the area mode function.

NOTE

- The area mode function is released when the power is turned off or when a video is played back.

Top of the page