- Top
- Menu Operations
- Menu list
- [OUTPUT SEL]

# [OUTPUT SEL]

Configure the settings regarding video output from <SDI OUT>, <HDMI OUT>, <GENLOCK IN/VIDEO OUT>, or <TC IN/OUT> terminal.

Item | Description of settings
--- | ---
[SDI OUT] | Selects video output from the <SDI OUT> terminal. [ON]: Outputs video. [OFF]: Does not output video. Factory setting: [OFF]
[SDI&HDMI SELECT] | Selects output signals from the <SDI OUT> terminal and <HDMI OUT> terminal. [SYSTEM MODE]: Follows the setting in [SYSTEM MODE] → [LINE&FREQ]. [1080i]: Converts into interlaced signals and outputs them when [1080-59.94P] or [1080-50P] is selected in [SYSTEM MODE] → [LINE&FREQ]. This cannot be selected when other settings are made. [DOWNCON]: Down converts to SD signal and outputs. Factory setting: [SYSTEM MODE]
[3G-SDI OUT] | Selects 1080P signals of the HD SDI output in 1080P mode. [LEVEL-A]: Selects the LEVEL-A method. [LEVEL-B]: Selects the LEVEL-B DL method. Factory setting: [LEVEL-B]
[SDI OUT CHAR] | Selects whether to superimpose characters on <SDI OUT> terminal output images. [ON]: Superimposes. [OFF]: Does not superimpose. Factory setting: [OFF]
[SDI EDH] | Selects whether to superimpose EDH when output from the <SDI OUT> terminal is SD signal (480i and 576i). [ON]: Superimposes. [OFF]: Does not superimpose. Factory setting: [ON]
[HD SDI REMOTE] | Sets whether to use the control function of recording operation for an external device (such as a recorder) connected to the <SDI OUT> terminal at HD SDI output. [ON]: Controls the recording operation of the external device. [OFF]: Does not control the recording operation of the external device. Factory setting: [OFF]
[DOWNCON MODE] | Selects the mode of the down converter output signal mode from the <SDI OUT> or <GENLOCK IN/VIDEO OUT> terminal in HD mode (1080P, 1080i, or 720P). [SIDE CROP], [LETTER BOX], [SQUEEZE] Factory setting: [LETTER BOX]
[DOWNCON SETTING] | [DETAIL] | Turns detail function for the down converter output signal [ON]/[OFF]. [ON], [OFF] The down converter output signal contains detail components set during HD signal processing. This setting superimposes the detail components exclusive to down converter output to that signal. Factory setting: [ON]
| [H.DTL LEVEL] | Sets horizontal detail correction level for the down converter output signal. [0]…[31] Factory setting: [8]
| [V.DTL LEVEL] | Sets vertical detail correction level for the down converter output signal. [0]…[31] Factory setting: [4]
| [DTL CORING] | Sets the detail noise removal level. [0]…[15] Factory setting: [1]
| [H.DTL FREQ] | Selects the horizontal detail frequency. [2.5MHz], [3MHz], [3.5MHz], [4MHz], [4.5MHz] Factory setting: [3.5MHz]
[VIDEO OUT] | Selects the <GENLOCK IN/VIDEO OUT> terminal output [ON]/[OFF]. [ON]: Performs output. [OFF]: Stops output. Factory setting: [OFF]
[VIDEO OUT CHAR] | Selects whether to superimpose characters on <GENLOCK IN/VIDEO OUT> terminal output images. [ON]: Superimposes. [OFF]: Does not superimpose. Factory setting: [ON]
[VIDEO OUT ZEBRA] | Selects whether the zebra pattern is superimposed over the output video signals from the<GENLOCK IN/VIDEO OUT> terminal. [ON]: Superimposes. [OFF]: Does not superimpose. Factory setting: [OFF]
[TC OUT] | Sets the type of time code output from the <TC IN/OUT> terminal. [TCG]: Outputs the time code generator value of the camera at all times. [TCG/TCR]: Outputs the time code generator value for camera image output, and the time code value of the video being played back for video playback output. Factory setting: [TCG]
[TC OUTPUT REF] | Sets the output delay of time code output from the <TC IN/OUT> terminal. [RECORDING]: Outputs the recorded time code with no delay. This is used when performing simultaneous recording on two cameras with the time code of this camera as the master. [VIDEO OUT]: Matches to output images. Factory setting: [VIDEO OUT]

Top of the page