- Top
- Shooting
- Dual codec recording
- Error displays about proxy data recordings

# Error displays about proxy data recordings

If an error occurs during recording the proxy data, check the entries in the following table and take necessary actions.

Error displays (viewfinder screen) | Behavior and cause | Action to take
--- | --- | ---
[PROXY ERROR] or [PROXY REC WARNING] | Proxy data recording will stop, but recording of the material will continue. An error occurred in the internal proxy module. [PROXY ERROR] A proxy data recording error occurred. [PROXY REC WARNING] If a proxy data recording error occurs, the proxy data currently being recorded will be processed as below: The proxy data being recorded to the P2 card will be deleted. The proxy data being recorded to the SD memory card will not be restored. | The proxy data will not be properly recorded. Turn off the camera and turn on it again to check the recording and playback. If the error continues to occur, please consult your dealer.
[SD 0 min] | Recording of the materials and proxy data will continue. The remaining SD memory card capacity is getting low. (approximately shorter than one minute) | After finishing recording, insert a new SD memory card.
[SD END] | Proxy data recording to the SD memory card will stop, but recording to the P2 card will continue. No SD memory card capacity remains. | After finishing recording, insert a new SD memory card. The proxy data being recorded to the SD memory card will be deleted. To restore the deleted proxy data, select clips in the P2 card and copy them to the SD memory card. (Copying proxy data to the SD memory card)
[SD WR ERR] | Proxy data recording to the SD memory card will stop, but recording to the P2 card will continue. This is displayed when proxy data cannot be recorded in the SD memory card even though [PROXY REC(P2&SD)] is set in main menu → [RECORDING SETUP] → [DUAL CODEC SETTING] → [CODEC USAGE]. #### If the error message is displayed when recording starts: The SD memory card format is different. The SD memory card contains 1000 clips or more. #### If the error message is displayed during recording: The SD memory card was ejected during recording. An error occurred in recording to the SD memory card. | Check the status of the SD memory card and insert a recordable card. (Checking the SD memory card)
[SD --min] or [SD WP] | Proxy data will not be recorded to the SD memory card, but recording to the P2 card will be performed. No SD memory card is inserted. [SD --min] The SD memory card is write-protected. [SD WP] | Check the status of the SD memory card.

## Copying proxy data to the SD memory card

Press the <THUMBNAIL> button to display the thumbnail screen.

Use the control stick to move the cursor to the clip to be copied and press the control stick.

Select [SD CARD] in the main menu → [CLIP] → [COPY].

Select [YES] in the confirmation message and press the control stick.

NOTE

- If [SD END] is displayed and the proxy data being recorded to the SD memory card is deleted, perform this procedure to copy the proxy data from the P2 card, and enable the deleted proxy data to be restored.

- Source data is not copied.

Top of the page