- Top
- Network Connection
- Using FTP client function
- Writing back from an FTP server to an SD memory card (import)

# Writing back from an FTP server to an SD memory card (import)

You can write back the selected folders from an FTP server on the network to an SD memory card.

Display the FTP explorer screen.

The folders of the server that has been set are displayed.

Select folders to be written back.

Select [SD CARD] in the main menu → [CLIP] → [IMPORT].

Press the control stick.

A confirmation message appears. Select [OK] to start writing back to the SD memory card.

When writing back is completed, [COPY COMPLETED!] appears.

NOTE

- To cancel the writing back process, press the control stick. Select [YES] when a [CANCEL] confirmation message appears, and then press the control stick. Files partially written back in the SD memory card are deleted, but successfully written files remain.

- After writing starts, disconnection errors will no longer be detected. Cancel the import operation if the copying progress has stalled.

- Depending on factors such as the number or sizes of files in the selected folder, and network conditions, writing back may take time.

- Any files with the same path names as the one in the SD memory card will be overwritten. However, if the path names are the same but the types differ (folder and file), an error is generated.

- To prevent unintended overwriting, format the SD memory card before writing back whenever possible.

- To transfer clips using SSH, the FTP server must support SSH.

- Using SSH will reduce the transfer speed.

Top of the page