- Top
- Description of Parts
- Right side

# Right side

1. Eye cup (Attaching the eye cup)

2. Eye piece

3. Busy (active status indication) lamp (Removing SD memory cards)

   Indicate the active status of the SD memory card, and is illuminated when the card is active.

4. SD memory card slot (Inserting SD memory cards)

   This is the insertion slot for the SD memory card (optional). Use the SD memory card for recording/opening the setting menu of the camera, or uploading metadata or proxy recording, etc.

   NOTE

   - Cautions when using SD memory cards

     - On the camera, use SD memory cards that conform to the SD standard, SDHC standard, or the SDXC standard. To record the proxy data, use SD, SDHC, or SDXC memory cards with an indication of class2 or higher.

       If the recording format of the proxy data is [SHQ 2CH MOV] or [AVC-G6 2CH MOV], use a card of class4 or higher.

     - MMC (Multi Media Card) cannot be used. (Bear in mind that taking pictures may no longer be possible if you use them.)

     - When using miniSD/microSD cards with the camera, always install the adaptor specially designed for miniSD/microSD cards. (The camera will not work properly if only the miniSD/microSD adaptor is installed. Make sure that the card has been inserted into the adaptor before use.)

     - Use of Panasonic SD memory cards and miniSD/microSD cards is recommended. Be sure to format cards on the camera before use.

     - Refer to our support desk at the following website for the latest information not included in these operating instructions.

       https://pro-av.panasonic.net/

     - SDHC memory cards are a standard that was established in 2006 by the SD Association for large-capacity memory cards that exceed 2 GB.

     - SDXC memory cards are a standard that was established in 2009 by the SD Association for large-capacity memory cards that exceed 32 GB.

5. Recording button (grip side) (Shooting)

   Press this button to start recording. Press it again to stop recording.

   Used for direct shooting in thumbnail mode.

6. Power switch (Preparation)

   Switch on/off the power.

7. Microphone cable clamp (Attaching the front microphone)

   Used for securing the microphone cable.

8. Pin holder

   Attach the zoom ring pin which is removed from the camera.

9. Headphones terminal (Headphones)

   This is the connecting terminal of headphones for audio monitor.

10. <AUDIO INPUT 2> terminal (XLR, 3-pin) (Using the external microphone and audio device)

    Connect the audio equipment or the microphone.

11. <SDI OUT> terminal (Supplying the time code externally)

    This is the output terminal for HD/SD SDI signals.

12. <TC IN/OUT> terminal (Definition of time data)

    This is the input/output terminal for time code.

    Use the <IN/OUT> switch to select the input or output.

13. <GENLOCK IN/VIDEO OUT> terminal (Externally locking the time code)

    This is the input terminal for reference signals when setting the genlock to the camera section. This is the output terminal of the video for monitor.

    Use the <IN/OUT> switch to switch the input or output.

14. <IN/OUT> switch (User bits settings)

    Switch the input and output of the <TC IN/OUT> terminal and <GENLOCK IN/VIDEO OUT> terminal.

15. <CAM REMOTE> terminal (Remote control)

    Connect the remote control (optional) to control some functions remotely.

    <FOCUS IRIS>: (3.5 mm mini jack) Control the focus operation and iris operation remotely.

    <ZOOM S/S>: (2.5 mm mini jack) Control the zoom operation and start/stop operation of recording remotely.

16. Tripod holes

    Attach the tripod. (bottom)

    - Mounting hole size

      - 1/4-20 UNC (screw length 5.5 mm or shorter)

      - 3/8-16 UNC (screw length 5.5 mm or shorter)

17. <OPEN> button (For the wireless module AJ-WM30/AJ-WM50)

    Use this button when opening the cover of the <USB2.0 HOST> terminal at the bottom of the button.

18. <USB2.0 HOST> terminal (sub-host) (For the wireless module AJ-WM30/AJ-WM50)

    This is the terminal for the wireless LAN. Mount the wireless module AJ-WM30/AJ-WM50 (optional).

Top of the page