- Top
- Shooting
- Setting the time data
- Supplying the time code externally

# Supplying the time code externally

You can supply the output time codes to a VTR or other recording device from the camera by matching the camera images or the replayed images.

<GENLOCK IN/VIDEO OUT> terminal or <SDI OUT> terminal

VIDEO IN terminal

SDI IN terminal

HD SDI IN terminal

VTR, etc.

TC IN terminal

<TC IN/OUT> terminal

Set [VIDEO OUT] in the main menu → [OUTPUT SEL] → [TC OUTPUT REF].

Set to [HD SDI] or [COMPOSITE] depending on the video output supplied with the main menu → [OTHER FUNCTIONS] → [GL PHASE].

Set [TCG/TCR] in the main menu → [OUTPUT SEL] → [TC OUT].

NOTE

- If you set [TC OUTPUT REF] to [VIDEO OUT] in the main menu → [OUTPUT SEL], the input time code will be output to match the video output delay.

Top of the page