- Top
- Description of Parts
- Front side, rear side

# Front side, rear side

1. Built-in microphone (Using the built-in microphone)

   This is the built-in stereo microphone.

2. Light sensor

   Detects indoor and outdoor light.

3. Front tally lamp (Tally lamp)

   Lights during shooting. This lamp will blink when the battery level becomes low.

4. Recording button (front side) (Shooting)

   Press this button to start recording. Press it again to stop recording.

   The operation of this button can be forbidden by the main menu → [SW MODE] → [FRONT REC].

5. <AWB> button (Adjusting the white balance)

   Press this button to adjust the white balance. Press it for two seconds or more to adjust the white balance and then black balance.

6. Eye sensor (Using the viewfinder)

   Bring your eyes closer to display the screen on the viewfinder.

   NOTE

   - The eye sensor may not work properly depending on the shape of glasses in use, how you hold the camera, or by hitting the strong light around the eye piece.

7. Viewfinder (Adjusting and setting the viewfinder)

8. <AUDIO INPUT 1> terminal (XLR, 3-pin) (Attaching the front microphone)

   Connect the audio equipment or the microphone.

9. Rear tally lamp (Tally lamp)

   Light during shooting. This lamp will blink when the battery level becomes low.

10. Battery attachment (Attaching and removing the battery)

11. Battery release button (Attaching and removing the battery)

    Remove the battery.

12. microP2 memory card 1 access LED (P2 card access LEDs and status of P2 cards)

    Indicate the access status of recording and playback of the card inserted in the microP2 memory card slot 1.

13. microP2 memory card slot 1 (Inserting a P2 card)

14. microP2 memory card 2 access LED (P2 card access LEDs and status of P2 cards)

    Indicate the access status of recording and playback of the card inserted in the microP2 memory card slot 2.

15. microP2 memory card slot 2 (Inserting a P2 card)

16. P2 memory card slot (Inserting a P2 card)

17. P2 memory card access LED (P2 card access LEDs and status of P2 cards)

    Indicate the access status of recording and playback of the card inserted in the P2 memory card slot.

18. <AUDIO OUT> terminal (TV/monitor)

    Output audio signals recorded to audio channel 1/2.

19. <USB3.0 HOST> terminal (host) (Connecting to external devices in USB host mode)

    Connect external hard disk drive, etc.

20. <USB2.0 DEVICE> terminal (device) (Connecting to a computer in the USB device mode)

    Connect to a computer with the USB 2.0 cable to transfer data.

21. <HDMI OUT> (monitor output) terminal (TV/monitor)

    This is the output terminal of the video for monitor.

22. <LAN> terminal (For wired LAN)

    Connect the LAN cable.

23. <DC IN 12V> terminal (Using the AC adaptor)

    This is the input terminal for the external power supply. Connect the supplied AC adaptor.

Top of the page