- Top
- Menu Operations
- Menu list
- [DISPLAY SETUP]

# [DISPLAY SETUP]

Configure the settings regarding the details to be displayed on the viewfinder or LCD monitor.

These menu items cannot be set when the thumbnail screen is displayed.

Item | Description of settings
--- | ---
[MENU DISPLAY] | Selects the LCD monitor or the view finder as the location where the menu is displayed. [LCD&EVF]: Displays the menu both on the LCD monitor and the viewfinder. [LCD]: Displays the menu only on the LCD monitor. Factory setting: [LCD&EVF]
[ZEBRA1 DETECT] | Sets the extraction level of zebra pattern 1. [0%]…[109%] Factory setting: [70%]
[ZEBRA2 DETECT] | Sets the extraction level of zebra pattern 2. [0%]…[109%] Factory setting: [85%]
[ZEBRA2] | Sets on/off of zebra pattern 2 and selects the type. [ON], [SPOT], [OFF] Factory setting: [SPOT]
[CENTER MARK] | Controls the center mark. [1]: + (large) [2]: Open center (large) [3]: + (small) [4]: Open center (small) [OFF]: Does not display. Factory setting: [1]
[SAFETY MARK] | Selects the type of frame for the safety zone marker. [1]: Box [2]: Corners [OFF]: Does not display. Factory setting: [2]
[SAFETY AREA] | Sets the size of the safety zone marker. The constant ratio of length to width can be set in 1% increments. [80%]…[100%] Factory setting: [90%]
[FRAME MARK] | Enables/disables frame marker. [ON], [OFF] Factory setting: [OFF]
[FRAME SIG] | Sets frame marker aspect ratio. [4:3], [13:9], [14:9], [1.85:1], [2.35:1] Factory setting: [4:3]
[FRAME LVL] | Sets the level of the outside of the frame marker. [0]…[15] Factory setting: [15]
[LEVEL GAUGE] | Enables/disables level gauge. [ON], [OFF] Factory setting: [OFF]
[FOCUS BAR] | Displays/hides the focus bar indicating the degree of focus. [ON], [OFF] Factory setting: [OFF]
[ZOOM/FOCUS] | Selects the unit of zoom and focus values. [NUMBER]: Displays position values of zoom and focus from [0] to [99]. [mm/feet]: Zoom is displayed in units of millimeters, and focus in units of feet. [mm/m]: Zoom is displayed in units of millimeters, and focus in units of meters. [OFF]: Neither zoom nor focus is displayed. Factory setting: [NUMBER]
[LEVEL METER] | Displays/hides audio level meter. [ON], [OFF] Factory setting: [ON]
[DATE/TIME] | Sets date and time display. [TIME]: Displays the hour, minute, and second. [DATE]: Displays the year, month, and date. [TIME&DATE]: Displays the hour, minute, and second, as well as year, month, and date. [OFF]: Does not display. Factory setting: [OFF]
[REC COUNTER] | Sets operation of the counter for recording. [TOTAL]: Performs continuous counting until it is reset using the <RESET> button. [CLIP]: Clears the counter value at the start of recording and counts the time for each recording. Factory setting: [TOTAL]
[P2CARD REMAIN] | Turns display of the remaining recording capacity for the P2 card [ON]/[OFF]. [ON], [OFF] Factory setting: [ON]
[BATTERY] | Turns the battery charge level indicator [ON]/[OFF]. [ON], [OFF] Factory setting: [ON]
[REC DURING UPLOAD] | Selects [ON]/[OFF] of the rec during upload display status. [ON], [OFF] Factory setting: [ON]
[STREAMING] | Selects [ON]/[OFF] indicating the distribution status of the streaming video. [ON], [OFF] Factory setting: [ON]
[OTHER DISPLAY] | Sets display details of other information. [PARTIAL]: Displays information partly. [ALL]: Displays all information. [USER]: Displays the information set in [DISPLAY SETTING]. Factory setting: [PARTIAL]
[DISPLAY SETTING] | [IRIS] | Displays/hides F value and auto iris control status. [ON], [OFF] Factory setting: [ON]
| [GAIN] | Displays/hides gain value. [ON], [OFF] Factory setting: [ON]
| [SHUTTER] | Displays/hides shutter speed. [ON], [OFF] Factory setting: [ON]
| [WHITE BALANCE] | Displays/hides the <WHITE BAL> switch position. [ON], [OFF] Factory setting: [ON]
| [ND] | Displays/hides the set value of ND filter. [ON], [OFF] Factory setting: [ON]
| [Y GET] | Displays/hides brightness of Y GET. [ON], [OFF] Factory setting: [ON]
| [D.ZOOM] | Displays/hides digital zoom display. [ON], [OFF] Factory setting: [ON]
| [SCENE FILE] | Displays/hides scene file name. [ON], [OFF] Factory setting: [ON]
| [DRS] | Toggles whether to display when the dynamic range stretcher function is activated. [ON], [OFF] Factory setting: [ON]
| [FBC] | Toggles whether to display when the flash band compensation function is activated. [ON], [OFF] Factory setting: [ON]
| [AREA] | Toggles whether to display when the area mode function is activated. [ON], [OFF] Factory setting: [ON]
| [OIS] | Displays/hides image stabilizer display. [ON], [OFF] Factory setting: [ON]
| [FULL AUTO] | Displays/hides the display when the <AUTO/MANUAL> switch is at <AUTO>. [ON], [OFF] Factory setting: [ON]
| [SHOOTING MODE] | Displays/hides high-sensitivity mode. [ON], [OFF] Factory setting: [ON]
| [PB MODE] | Displays/hides the operation status of playback. [ON], [OFF] Factory setting: [ON]
| [SYSTEM MODE] | Displays/hides system mode. [ON], [OFF] Factory setting: [OFF]
| [REC FORMAT] | Displays/hides recording format display. [ON], [OFF] Factory setting: [ON]
| [FRAME RATE] | Displays/hides frame rate. [ON], [OFF] Factory setting: [ON]
| [ASPECT] | Displays/hides letterbox recording display. [ON], [OFF] Factory setting: [ON]
| [REC MEDIA] | Displays/hides recording media. [ON], [OFF] Factory setting: [ON]
| [ONE CLIP REC] | Displays/hides the status of one-clip recording mode. [ON], [OFF] Factory setting: [ON]
| [REC MODE] | Displays/hides simultaneous recording mode display. [ON], [OFF] Factory setting: [ON]
| [PROXY] | Displays/hides proxy information. [ON], [OFF] Factory setting: [ON]
| [GPS] | Displays/hides GPS signal reception status. [ON], [OFF] Factory setting: [ON]
[EVF DETAIL] | Adjusts the contour of the video in the viewfinder or LCD monitor to make it easier to focus. [ON], [OFF] Factory setting: [ON] If the function is assigned to the USER button, [ON]/[OFF] can be switched using the USER button.
[EVF PEAK LEVEL] | Adjusts the peaking level of the viewfinder and LCD monitor. [−7]…[7] Factory setting: [0]
[EVF PEAK FREQ] | Adjusts the peaking frequency of the viewfinder and LCD monitor. [HIGH], [LOW] Factory setting: [LOW]
[EVF SETTING] | [EVF BRIGHTNESS] | Adjusts the brightness of the viewfinder. [−15]…[15] Factory setting: [0]
| [EVF CONTRAST] | Adjusts the contrast of the viewfinder. [−30]…[30] Factory setting: [0]
| [EVF COLOR LEVEL] | Adjusts the color level of the viewfinder. [−15]…[15] Factory setting: [0]
| [EVF COLOR] | Selects whether to display video in the viewfinder in color or in black and white. [ON]: Displays in color. [OFF]: Displays in black and white. Factory setting: [ON]
[EYE SENSOR] | Selects sensitivity of eye sensor. [HIGH], [LOW] Factory setting: [HIGH]
[LCD SETTING] | [LCD BRIGHTNESS] | Adjusts the brightness of the LCD monitor. [−15]…[15] Factory setting: [0]
| [LCD CONTRAST] | Adjusts the contrast of the LCD monitor. [−30]…[30] Factory setting: [0]
| [LCD COLOR LEVEL] | Adjusts the color level of the LCD monitor. [−15]…[15] Factory setting: [0]
| [LCD BACKLIGHT] | Adjusts the brightness of the LCD monitor backlight. [1]…[−3] [1]: Brightens more than normal. [−3]: Becomes the darkest. Factory setting: [0]
[SELF SHOOT] | Sets the display of the LCD monitor when mirror shooting is performed. [NORMAL]: Does not invert the left and right sides. [MIRROR]: Inverts the left and right sides. Factory setting: [MIRROR]

Top of the page