- Top
- Shooting
- Multi formats
- Selecting video output

# Selecting video output

The video output method can be selected.

Video output, etc. can be selected by the setting of [SDI&HDMI SELECT], [3G-SDI OUT], or [DOWNCON MODE] in the main menu → [OUTPUT SEL].

Item | Description of settings
--- | ---
[SDI&HDMI SELECT] | Selects output signals from the <SDI OUT> terminal and <HDMI OUT> terminal.
[3G-SDI OUT] | Selects the 3G-HD SDI signal type output from the <SDI OUT> terminal from [LEVEL-A] and [LEVEL-B] at 1080P.
[DOWNCON MODE] | Selects the mode of the down converter output signal from the <SDI OUT> or <GENLOCK IN/VIDEO OUT> terminal in HD mode (1080P, 1080i, 1080/23.98PsF, or 720P).

## Selecting video output from each terminal

- “—” indicates an item that cannot be selected.

Setting | Video output
--- | ---
[LINE&FREQ] | [SDI&HDMI SELECT] | <SDI OUT> terminal | <HDMI OUT> terminal | <GENLOCK IN/VIDEO OUT> terminal
[1080-59.94P] | [SYSTEM MODE] | 1080/59.94P*1 | 1080/59.94P | 480/59.94i
[1080i] | 1080/59.94i | 1080/59.94i | 480/59.94i
[DOWNCON] | 480/59.94i | 480/59.94P | 480/59.94i
[1080-50P] | [SYSTEM MODE] | 1080/50P*2 | 1080/50P | 576/50i
[1080i] | 1080/50i | 1080/50i | 576/50i
[DOWNCON] | 576/50i | 576/50P | 576/50i
[1080-59.94i] | [SYSTEM MODE] | 1080/59.94i | 1080/59.94i | 480/59.94i
[DOWNCON] | 480/59.94i | 480/59.94P | 480/59.94i
[1080-50i] | [SYSTEM MODE] | 1080/50i | 1080/50i | 576/50i
[DOWNCON] | 576/50i | 576/50P | 576/50i
[1080-23.98PsF] | [SYSTEM MODE] | 1080/23.98PsF*2 | — | 480/59.94i
[DOWNCON] | 480/59.94i | — | 480/59.94i
[720-59.94P] | [SYSTEM MODE] | 720/59.94P | 720/59.94P | 480/59.94i
[DOWNCON] | 480/59.94i | 480/59.94P | 480/59.94i
[720-50P] | [SYSTEM MODE] | 720/50P | 720/50P | 576/50i
[DOWNCON] | 576/50i | 576/50P | 576/50i
[480-59.94i] | — | 480/59.94i | 480/59.94P | 480/59.94i
—
—
[576-50i] | — | 576/50i | 576/50P | 576/50i
—
—

Output type can be selected from [LEVEL-A] and [LEVEL-B] in the main menu → [OUTPUT SEL] → [3G-SDI OUT]. [LEVEL-B] is set in the factory settings.

When [LINE&FREQ] is set to [1080-23.98PsF] and [SDI&HDMI SELECT] is set to [SYSTEM MODE], video output from the <SDI OUT> terminal in thumbnail mode or playback mode (including recording check) becomes 1080/60P. In addition, it is not output from the <HDMI OUT> terminal. When the mode is changed between the camera mode and thumbnail mode (or playback mode), video signal output from the <SDI OUT> terminal and the <GENLOCK IN/VIDEO OUT> terminal may be disrupted, or video on the LCD monitor and viewfinder may be disrupted.

Top of the page