- Top
- Connecting to External Devices
- Connection function via <USB2.0 DEVICE> or <USB3.0 HOST> terminal
- Connecting to external devices in USB host mode

# Connecting to external devices in USB host mode

You can save data on cards or other operations by connecting a storage device such as hard disk drive or solid-state drive that can be connected via USB 2.0 or USB 3.0 to the <USB3.0 HOST> terminal.

## Switching to the USB host mode

USB cable (optional)

External storage device

Fig. 1

Fig. 2

Fig. 3

Connect the storage device to the <USB3.0 HOST> terminal. (Fig. 1)

- When connecting a storage device which supports USB 3.0, use a cable that conforms to the USB 3.0 standard.

- When a USB 2.0 cable is used, the transfer rates cannot be faster than the ability of USB 2.0.

- If the storage device is recognized and is usable, (gray) on the top right of the thumbnail screen changes to (white).

Set to [STORAGE] in the main menu → [NETWORK SETUP] → [USB MODE SELECT]. (Fig. 2)

For details, refer to “Setting menu basic operations”.

Set [ON] in the main menu → [NETWORK SETUP] → [USB MODE]. (Fig. 3)

- The camera is switched to the USB host mode.

- While in USB host mode, [USB STORAGE CONNECTED] is displayed in the center of the viewfinder or LCD monitor. If the USB connection is being moved or the hard disk drive is not connected properly, [USB STORAGE CONNECTING...] is displayed.

Press the <THUMBNAIL> button.

- The thumbnail screen is displayed.

- Ensure that [USB] is displayed at the top right of the screen.

- If a storage device is connected, the icon that indicates storage device status at the top right illuminates. However, a red mark indicates that the device cannot be used.

  For details on USB host mode, refer to “Connecting to external devices in USB host mode”.

Exit the USB host mode.

There are two methods:

- Turn the power switch of the camera to <OFF>.

- With the thumbnail screen closed, set [OFF] in the main menu → [NETWORK SETUP] → [USB MODE].

- Press the USER button to which [USB MODE] has been assigned. Note that this is disabled when a menu or thumbnail is open.

NOTE

- In USB host mode, a P2 card can be played back. Camera image and external input cannot be recorded.

  Clips written to the hard disk drive cannot be played back on the camera.

- A storage device cannot be connected to the <USB2.0 HOST> terminal (<USB2.0 HOST> terminal (sub-host)).

- While connecting a storage device, use the fully charged battery or connect an AC adaptor to the camera to avoid problems in copying or formatting operations.

- The <USB3.0 HOST> terminal also supports USB bus power (5 V, 0.9 A). However, there are certain devices that cannot run depending on the storage device used. In such cases, add a separate power supply to the storage device.

- Some storage devices may not function properly depending on the storage device and cable used.

- Do not connect multiple storage devices using a hub even if the storage devices are turned off. Do not connect other devices together with your storage device using a hub.

- During a format or copy operation, do not unplug the cable, eject the target P2 card, or turn off the camera or the storage device. Rebooting the camera and the storage device is required.

- A storage device with the SATA (Serial ATA) or PATA (Parallel ATA) interface connected using a USB conversion cable may not be recognized.

- Do not connect or disconnect the cable during playback on the camera. Playback may not be performed properly.

## Storage device types and available functions

The available functions differ depending on the storage device you will use. The storage device type is displayed after [PARTITION] on the left side of the storage device explorer screen.

For details, refer to “Storage device information display (explorer screen)”.

#### Storage device type

Storage device type | Features
--- | ---
[TYPE S] | A special format to read/write data with high speed by card.
[P2STORE] | Indicates P2 STORE (AJ-PCS060G). Writing is disabled.
[FAT] | Storage devices where the primary partition is FAT16 or FAT32. The partition root or CONTENTS folder under any folders* is the target.
[OTHER] | Indicates other storage devices other than the above. File systems other than FAT16 and FAT32, such as NTFS.

The hierarchy of folders is down to the third level and the maximum number of folders is 100. Long file names and file names with double-byte characters are not supported. Examples of folder displays are shown below.

/CONTENTS | Can be displayed.
/SAMPLE/CONTENTS | Can be displayed.
/SAMPLE/20140101/CONTENTS | Can be displayed.
/SAMPLE/20140101/1200/CONTENTS | Cannot be displayed. (Cannot be displayed since this is a fourth level folder)

#### Storage device types and available functions

Available functions | Storage device type
--- | ---
[TYPE S] | [P2STORE] | [FAT] | [OTHER]
Thumbnail display | ✓ | ✓ | ✓ | —
Card unit | Card*1 → Storage | ✓ | — | ✓ | —
Card*2 → Storage | — | — | — | —
Storage → Card*1 | ✓ | ✓ | — | —
Storage → Card*2 | — | — | — | —
Clip unit | Card → Storage | ✓*4 | — | ✓ | —
Storage → Card | ✓ | ✓ | ✓ | —
Playback check*3 | — | — | — | —
Clip image display | ✓ | ✓ | ✓ | —
Format | ✓ | — | ✓ | ✓*5

P2 memory card, or microP2 memory card with 32 GB or lower

microP2 memory cards that exceed 32 GB

Playback from the storage device cannot be performed on the camera. Import the contents to the P2 card to play them back.

If you perform additional clip writing, you will not be able to write back to that partition by card.

Storage devices with a capacity of 2 TB or more cannot be formatted.

NOTE

- Storage devices with capacities exceeding 2 TB (2048 GB) are not supported.

- Use a storage device within its guaranteed operational range (temperature, etc.).

- Do not place the storage device in a location that is unstable or subject to vibration.

- Use a storage device with sufficient capacity for copying.

- Because the storage device is very sensitive, reading, and writing data may become invalid depending on your usage. Please note that Panasonic has no responsibility for data loss caused from a storage device failure or other defects and any direct or indirect damage related to these.

- If the contents of the storage device used for copying data from the camera are replaced using another computer, the camera operations and storage device data cannot be guaranteed.

- For P2 cards containing defective clips, it is recommended that you copy data to a storage device after restoring in advance.

## Formatting a storage device

You can initialize the storage device to a usable format using the [TYPE S] or the [FAT] file system.

Fig. 1

Select [STORAGE] in the main menu → [CLIP] → [EXPLORE] and press the control stick.

This opens the explorer screen.

Select the desired format ([TYPE S], [FAT]) in the main menu → [CLIP] → [FORMAT(STORAGE)] and press the control stick. (Fig. 1)

Select [YES] in the confirmation message and press the control stick.

Select [YES] again when the confirmation message appears, and press the control stick.

This formats the storage device.

NOTE

- Formatting the storage devices erases all of its contents. Data cannot be recovered once it is formatted. Always check the data before formatting.

## Exporting to a storage device by card

You can export to a storage device (write to a storage device from a P2 card) by P2 card. The copy results and the maximum number of items that can be copied vary depending on format type of the storage device. You cannot perform copying once the capacity of the storage device is exceeded.

Fig. 1

#### [TYPE S]

A partition is created for each card, and all data included in the card are copied there. You can check the part numbers and serial numbers of the P2 cards that have been copied on the explorer screen of the camera.

The maximum number of items that can be copied is 23.

#### [FAT]

A folder is created for each card. All data included in the card are copied there. You can check the folder names in the explorer screen of the camera.

Folders are created in two levels; the date folders on the first level and the time folders on the second.

Example) August 30, 2013, 12:34:56: /13-08-30/12-34-56

The maximum number of items that can be copied is 100.

Select [EXPORT] in the main menu → [CLIP] and press the control stick.

Move the cursor to the card slot number of the copy source and press the control stick.

For [TYPE S], selecting [ALL SLOT] exports all cards currently inserted.

Select [YES] in the confirmation message and press the control stick.

Exporting begins. A progress bar appears during exporting. (Fig. 1)

[COPY COMPLETED!] will be displayed when exporting is completed.

NOTE

- For export with [TYPE S], P2 card data and copied data can be verified (compared) automatically after exporting. Verification at the time of export is enabled in the factory setting. When you set to disable verification at the time of export, exported data is not verified, and the time until export completes will shorten. To disable verification, set [VERIFY] to [OFF] in the main menu → [CLIP] → [STORAGE COPY SETUP]. For [FAT], verification is not performed regardless of this setting.

- To discontinue the export process, press the control stick. A [CANCEL] confirmation message will appear. Select [YES] and press the control stick.

- Even if you cancel the process during verification, copying to the P2 card will continue until it is completed.

- microP2 memory cards that exceed 32 GB cannot be exported and imported. Use copied clips.

## Copying to a storage device by clip

You can copy only the selected clips to a storage device.

Go to the thumbnail screen. Use the control stick to place the cursor on a clip you want to copy and press the control stick.

You can also select multiple clips.

Select [STORAGE] in the main menu → [CLIP] → [COPY] and press the control stick.

A list of folders or partitions in the storage device is displayed.

Select the copy destination and press the control stick.

Select [YES] in the confirmation message and press the control stick.

This starts the copying process. A progress bar is displayed during copying.

[COPY COMPLETED!] will be displayed when copying is completed.

NOTE

- When the storage device has a [FAT] file system, the folders displayed are as follows:

  - Root

  - Folders down to the third level including the CONTENTS folder

- To copy to a [TYPE S] storage device, one or more partitions are required. You can either format the storage device to [FAT] or perform copying after creating a partition through the export process.

- To cancel the copy process, use the control stick to place the cursor on [CANCEL] and press the control stick. A [CANCEL] confirmation message will appear. Select [YES] and press the control stick. Clips copied halfway to the copy destination are deleted.

- If you have copied clips to a [TYPE S] storage device, you will not be able to import to that partition by card. Also, the part number display of the card at that instance will display [UNKNOWN].

## Storage device information display (explorer screen)

You can perform the following operations in the explorer screen display.

- Storage device information display

- Storage device partition or folder thumbnail display and selection

- Target partition or folder selection

To display the explorer screen, select [STORAGE] in the main menu → [CLIP] → [EXPLORE] and press the control stick.

1. Storage device indicator

   This displays the connected / not connected status and the storage device type.

2. Display mode

   This indicates that the explorer screen of the storage device is currently displayed.

3. Device information

   For [TYPE S] and [P2STORE] (storage devices that allow reading/writing by card)

   [PARTITION] | [TYPE S]/[P2STORE]
   [VENDOR] | Vendor name
   [MODEL] | Model name
   [SIZE] | Total capacity (unit: GB)
   [USED] | Used capacity (unit: GB) Used P2 card area (unit: number of clips), maximum of 23
   [FREE CAP.] | Remaining capacity (unit: GB)
   [SELECTED PART.] | Number of partitions selected

   For [FAT] and [OTHER] (other storage devices)

   [PARTITION] | [FAT]/[OTHER]
   [VENDOR] | Vendor name
   [MODEL] | Model name
   [SIZE] | Total capacity (unit: GB)
   [FREE CAP.] | Remaining capacity (unit: GB)
   [SELECTED PART.] | Number of folders selected

4. Partition or folder information

   For [TYPE S] and [P2STORE] (partition information)

   | Displays a checkmark when a target partition is selected
   [NO.] | Partition number
   [MODEL] | P2 card model name
   [PARTITION NAME] | Name assigned to the partition
   [DATE] | Partition record date
   [TIME] | Partition record time
   [SERIAL] | P2 card serial number

   For [FAT] and [OTHER] (folder information)

   | Displays a checkmark when a target partition is selected
   [NO.] | Folder number
   [FOLDER NAME] | Folder name (excluding the CONTENTS folder)
   [DATE] | Folder creation date
   [TIME] | Folder creation time

   NOTE

   - For [TYPE S] storage devices, you can switch the display between the partition name and serial name using the control stick.

   - If there is an invalid partition in [P2STORE], the partition information is displayed in gray.

   - The remaining free space of the corresponding partition can be checked in the main menu → [CLIP] → [PROPERTY] → [FREE CAP. OF PARTITION].

## Selecting the target folder/partition in the explorer screen

You can display all clips included in the selected partition/folder as thumbnails by selecting partitions/folders as targets. You can display up to six partitions/folders. When the seventh partition/folder is specified, setting is disabled and a warning is displayed.

Fig. 1

In the explorer screen, place the cursor on the partition/folder.

Press and hold the control stick (for one second or more).

The partition/folder is selected and a checkmark is displayed. (Fig. 1)

The selected target partition/folder is valid until the storage device is disconnected or the power is turned off. To release the selected partition/folder, hold down the control stick (for one second or more) again on the selected partition.

Press the <CANCEL> button to deselect all partitions/folders.

NOTE

- In [TYPE S] storage devices, [MODEL] is [UNKNOWN] and clips recorded across other partitions will not be one normal clip. Copying clips to a [TYPE S] storage device changes the partition of the copy destination [MODEL] to [UNKNOWN].

- The partition name can be set when a [TYPE S] storage device is used. The partition name that has been set is displayed in [PARTITION NAME] on the explorer screen.

## Setting a partition name in the explorer screen

When the storage device is [TYPE S], the name (up to 20 characters) can be set to the partition. The preset partition name is displayed in [PARTITION NAME] on the explorer screen.

In the explorer screen, place the cursor on the partition you want to set up.

You can display the thumbnail list and set names for partitions by pressing the control stick.

Select [CHANGE PARTITION NAME] in the main menu → [CLIP] and press the control stick.

This displays the soft keyboard.

Enter the partition name and select [OK].

The partition name is set.

## Deleting the last partition in the explorer screen

You can delete the last partition on a [TYPE S] type storage device.

In the explorer screen, place the cursor on the last partition.

Select [DELETE LAST PARTITION] in the main menu → [CLIP] and press the control stick.

NOTE

- You can only delete the last partition when using a [TYPE S] storage device. You can only delete the last partition. You cannot delete other partitions.

- Since deleted partitions cannot be recovered, perform a check thoroughly before deleting.

## Clip thumbnail display of the storage device

### Displaying thumbnails

You can display and manage clips saved in a storage device, as well as display the thumbnail screen for clips saved in a P2 card attached to the camera.

<SET>

<EXIT>

Open the explorer screen.

Partitions or folders are displayed in a list.

Use the control stick to place the cursor on the partition or folder you want to display on the thumbnail screen, and press the control stick.

This displays the thumbnails of clips in the partition or folder. You can go back to the main explorer screen by clicking the <EXIT> button.

NOTE

- When target partitions are selected, you can display thumbnails in all partitions selected as targets by pressing the control stick while holding down the <SHIFT> button.

#### Information display items

1. Storage device information

   For [TYPE S]

   [SERIAL] | P2 card serial number
   [MODEL] | P2 card model name
   [SELECTED PART.] | Displays a checkmark when a target partition is selected
   [SELECTED PART. NO.] | List of selected partition numbers (only displayed when multiple partitions are selected)
   [NO.] | Partition number
   [DATE] | Partition record date
   [TIME] | Partition record time
   [VERIFY] | Verification settings and results during recording, [ON/FAILED] [ON/FAILED]: Verification performed. Items match. [ON/FINISHED]: Verification performed but no match found. (For [P2STORE], [−−] is displayed.) [OFF]: Verification not performed
   [NAME] | Partition name defined by the user
   [SIZE] | Total capacity of the storage device
   [USED] | Used storage device capacity
   [FREE CAP.] | Remaining storage device capacity

   For [FAT]

   [SELECTED PART.] | Displays a checkmark when a target partition is selected
   [SELECTED PART. NO.] | List of selected folder numbers (only displayed when multiple folders are selected)
   [NO.] | Folder number
   [DATE] | Folder creation date
   [TIME] | Folder creation time
   [FOLDER] | Folder name (creation date and time are not displayed in the root folder)
   [SIZE] | Total capacity of the storage device
   [FREE CAP.] | Remaining storage device capacity

NOTE

- You can change the thumbnail screen display if necessary.

- The 1001st clips onwards are not displayed.

### Displaying clip information

You can display metadata of clips saved in a storage device. The procedure to display is the same as that of the P2 card clip properties.

In the storage device thumbnail screen, move the cursor to the target clip.

Select [CLIP PROPERTY] in the main menu → [CLIP] → [PROPERTY] and press the control stick.

This cannot be modified.

### Deleting clips

You can delete unnecessary clips saved in a storage device.

In the storage device thumbnail screen, select the clip you want to delete.

Select [DELETE] in the main menu → [CLIP] and press the control stick.

Move the cursor to [YES] in the confirmation message and press the control stick.

NOTE

- You may not be able to delete clips with defective clip or unknown clip indicators.

## Writing back to the P2 card from a storage device (import)

### Importing from a [TYPE S] storage device or [P2STORE] by partition

You can import (write back to a P2 card from as storage device) to a P2 card with the same part number as the source card by partition (card).

Insert a P2 card that will serve as the input destination.

Make sure to insert a formatted P2 card.

Connecting a storage device.

Select [STORAGE] in the main menu → [CLIP] → [EXPLORE] to display the explorer screen.

In the explorer screen, display the partition thumbnails to be imported.

Select [IMPORT] in the main menu → [CLIP].

Place the cursor on the P2 card slot number of the import destination and press the control stick.

Start importing by selecting [YES] in the confirmation message.

[COPY COMPLETED!] will be displayed when importing is completed.

NOTE

- Importing to a P2 card that is different from the source P2 card may result in incomplete clips depending on the clips. In this case, use the reconnection function to reconfigure the clips. For details, refer to “Reconnecting incomplete clips”.

- You can select whether to perform verification at the time of copying in the main menu → [CLIP] → [STORAGE COPY SETUP] → [VERIFY].

- You cannot import by partition to a P2 card of a different model. Perform copying by clip instead.

### Copying to a P2 card by clip

You can specify a storage device clip and copy it to a P2 card.

Open the storage device thumbnail screen.

Select the clip you want to copy.

In the main menu → [CLIP] → [COPY] → [STORAGE] list, move the cursor over the copy destination and press the control stick.

Start importing by selecting [YES] in the confirmation message.

[COPY COMPLETED!] will be displayed when copying is completed.

Top of the page