- Top
- Display
- Screen status display
- Mode check display

# Mode check display

The camera settings and status can be displayed on the viewfinder or LCD monitor screen for check.

Each time the <DISP/MODE CHK> switch on the camera is pushed towards the <CHK> side, the five screens are switched.

[STATUS] screen display → [FUNCTION] screen display → [AUDIO] screen display → [USER SW] screen display → [META INFO] screen display → no display

Each screen is displayed for approximately five seconds. Pushing the <DISP/MODE CHK> switch towards the <CHK> side while the screen is displayed moves to the next screen.

## [FUNCTION] screen

Displays the video output status and information of the recording media.

[SDI OUT] | — | Displays the status of the signal output from the <SDI OUT> terminal.
[TYPE] | Displays the format of the signal output from the <SDI OUT> terminal by [HD-SDI]/[SD-SDI].
[CHAR] | Displays the superimposition status of characters selected in the main menu → [OUTPUT SEL] → [SDI OUT CHAR] by [ON]/[OFF].
[P2CARD STATUS] | — | Displays the status of the P2 card inserted in the card slot, remaining capacity, and total used capacity. The statuses of cards to be displayed are as follows: [ACTIVE]/[ACCESSING]/[INFO READING]/[FULL]/[PROTECTED]/[NOT SUPPORTED]/[FORMAT ERROR]/[AUTH NG]/[REC IMPOSSIBLE]/[NO CARD] For details, refer to “P2 card access LEDs and status of P2 cards”.
[TOTAL P2/mP2] | Displays the remaining capacity/total capacity totaled for slots 1 and 2 (or slots 3) and the recording media ([P2] or [mP2]).
[SLOT1] | Displays the status of the microP2 memory card in slot 1 and remaining capacity/total capacity.
[SLOT2] | Displays the status of the microP2 memory card in slot 2 and remaining capacity/total capacity.
[SLOT3] | Displays the status of the P2 memory card in slot 3 and remaining capacity/total capacity.
[PROXY] | [MEDIA] | Displays the media selection status for proxy recording. [P2]/[P2&SD]/[OFF]
[MODE] | Displays the setting status for proxy recording mode. [AVC-G6 2CH MOV]/[SHQ 2CH MOV]/[HQ 2CH MOV]/[LOW 2CH MOV]
[PROXY ERROR] | Displays the operation error on the proxy module.
[NETWORK] | [NETWORK] | Displays the status of network to be used and streaming status.

## [AUDIO] screen

Displays audio settings and the selection status of each recording channel.

[AUDIO] | [INT MIC] | Displays the built-in microphone status set in the main menu → [AUDIO SETUP] → [INPUT SETTING] → [INT MIC]. [STEREO]: Records audio from two directions in the front with the 2ch stereo microphone. [MONO]: This mode records clearer audio from the front by enhancing the directionality forward like a shotgun microphone. Audio recorded on the left and right are the same. [OFF]: Disables audio of the built-in microphone.
[AUDIO OUT] | Displays the audio input signal status set in the main menu → [AUDIO SETUP] → [OUTPUT SETTING] → [AUDIO OUT]. [CH1/CH2]/[CH1]/[CH2]/[CH3/CH4]/[CH3]/[CH4]
[A.IN] | [CH1/2/3/4] | Displays the input status of each channel. [INT(L)]/[INT(R)]/[INPUT1]/[INPUT2]
[LEVEL] | [CH1/2/3/4] | Displays the recording level adjustment method currently selected on each channel. [VR]: Displayed when manual adjustment using the adjustment dial is set. [MENU]: Displayed when manual adjustment using [LEVEL CONTROL CH3]/[LEVEL CONTROL CH4] is set in the main menu → [AUDIO SETUP] → [RECORDING CH SETTING]. [AUTO]: Displayed when automatic adjustment is set.
[F.VR] | [CH1/2/3/4] | Displays by [ON]/[OFF] whether the <F.AUDIO LEVEL> dial is enabled on the channel to which [VR] (manual adjustment by adjustment dial) is displayed in [LEVEL].
[LIMITER] | [CH1/2/3/4] | Displays the limiter settings of each channel.
[LOWCUT] | [CH1/2/3/4] | Displays the lowcut filter status of each channel.

## [USER SW] screen

Displays the assignment status of each USER button. For details, refer to “Assigning functions to the USER buttons”.

[OTHER ASSIGN] | [GAIN L] | Displays the gain value assigned to <L> of the <GAIN> switch.
[GAIN M] | Displays the gain value assigned to <M> of the <GAIN> switch.
[GAIN H] | Displays the gain value assigned to <H> of the <GAIN> switch.
[S.GAIN] | Enumerates and displays the gain value assigned as super gain.
[WHITE BAL A] | Displays the color temperature assigned to <A> of the <WHITE BAL> switch.
[WHITE BAL B] | Displays the color temperature assigned to <B> of the <WHITE BAL> switch.
[WHITE BAL PRE] | Displays the color temperature assigned to <PRST> of the <WHITE BAL> switch.
[USER SW] | [USER1] to [USER8] | Displays the assignment to the USER1 to USER8 buttons.

## [META INFO] screen

Display the information added as metadata.

[META INFO] | [POSITION] | Displays the information (latitude, longitude, altitude, date and time) acquired from GPS when the main menu → [OTHER FUNCTIONS] → [GPS] is set to [INTERNAL].
[ROLL] | Displays the horizontal inclination of the camera acquired by the level gauge as an angle. Setting the horizontal position as 0°, inclination to the left is indicated as a minus value, and inclination to the right is indicated as a plus value.
[PITCH] | Displays the vertical inclination of the camera acquired by the level gauge as an angle. Setting the vertical position as 0°, downward inclination is indicated as a minus value, and upward inclination is indicated as a plus value.

Top of the page