- Top
- Menu Operations
- [OPTION MENU] list
- [AWB PRE CONTROL]

# [AWB PRE CONTROL]

Change the output display or output value for the white balance preset value [3200K].

Item | Description of settings
--- | ---
[R Gain] | Displays the output of Rch of preset [3200K]. The color can be changed on the Rch axis by changing the output of Rch. [−400]…[400] Factory setting: [0]
[B Gain] | Displays the output of Bch of preset [3200K]. The color can be changed on the Bch axis by changing the output of Bch. [−400]…[400] Factory setting: [0]
[G AXIS] | Displays the output of G axis of preset [3200K]. The color can be changed on the G axis by changing the output of Rch/Bch. [−400]…[400] Factory setting: [0]

Top of the page