- Top
- Network Connection
- Network function
- Setting for connection with Remote Operation Panel (AK-HRP200G)

# Setting for connection with Remote Operation Panel (AK-HRP200G)

You can remotely control some functions by connecting the remote operation panel AK-HRP200G (optional) via an IP connection.

To remotely control the camera after connecting the AK-HRP200G using a LAN cable, configure the settings using the following procedures:

Configure the network settings of the AK-HRP200G.

For the network settings, use ROP setup software that is supplied with AK-HRP200G.

Configure the network settings of the camera.

Set [DISABLE] in the main menu → [NETWORK SETUP] → [LAN PROPERTY] → [DHCP], and refer to steps 1 to 2 in “Wired LAN settings” to configure the network settings.

Set each item in the camera’s main menu → [NETWORK SETUP] → [NETWORK FUNC] → [USER ACCOUNT].

[USER NAME]: Sets the user account name. (Factory settings: [guest])

[PASSWORD]: Sets the password. (Factory setting: [p2guest])

Enter up to 31 characters for the user account name, and 6 to 15 characters for the password.

Set the camera’s main menu → [NETWORK SETUP] → [NETWORK FUNC] → [IP REMOTE] to [ENABLE].

The camera will restart. The IP connection will be possible after the camera is started. The camera will also restart when [IP REMOTE] is set to [DISABLE]. The IP connection mode is canceled after the camera is started.

NOTE

- The following camera information is required to connect to the AK-HRP200G.

  - User account name

  - Password

  - IP address

  - Port number: 49152

- Use Ver.4.01.00 or later versions of the AK-HRP200G firmware.

- For details on the operations of ROP setup software, refer to the Operating Instructions of the AK-HRP200G.

- Use Ver.3.0.0.0 or later versions of ROP setup software.

Top of the page