- Top
- Shooting
- Setting the time data
- Connecting and setting the genlock and time code input/output

# Connecting and setting the genlock and time code input/output

The relationship of the connecting and settings between the genlock and time code input/output is shown in the table.

When the genlock input and the camera output phase match, ✓ is displayed, and when they do not match, × is displayed.

#### When the camera recording format is 1080P, 1080i

Camera usage conditions | Image and standard signals supplied externally | SDI | VIDEO | SDI | VIDEO
Genlock input | 1080i | SD (480i/576i)
Camera settings | [GL PHASE] | [HD SDI] | [COMPOSITE] | [HD SDI] | [COMPOSITE]
Genlock input and camera output phase | SDI output (HD) | ✓ | 90H advance | ✓ | 90H advance
Video output and SDI output (SD) | 90H delay | ✓ | 90H delay | ✓
Time code output | ✓ | ✓ | ✓ | ✓

#### When the camera recording format is 1080/23.98PsF

Camera usage conditions | Image and standard signals supplied externally | SDI
Genlock input | 1080/23.98PsF
Camera settings | [GL PHASE] | [HD SDI]
Genlock input and camera output phase | SDI output (HD) | ✓
Video output and SDI output (SD) | ×
Time code output | ✓

#### When the camera recording format is 720P

Camera usage conditions | Image and standard signals supplied externally | SDI | VIDEO | SDI | VIDEO
Genlock input | 720P | SD (480i/576i)
Camera settings | [GL PHASE] | [HD SDI] | [COMPOSITE] | [HD SDI] | [COMPOSITE]
Genlock input and camera output phase | SDI output (HD) | ✓ | 120H advance | ✓ | 120H advance
Video output and SDI output (SD) | 120H delay | ✓ | 120H delay | ✓
Time code output | × | × | ✓ | ✓

#### When the camera recording format is 480i/576i

Camera usage conditions | Image and standard signals supplied externally | SDI | VIDEO
Genlock input | SD (480i/576i)
Camera settings | [GL PHASE] | Disabled
Genlock input and camera output phase | SDI output (HD) | None
Video output and SDI output (SD) | ✓
Time code output | ✓

Top of the page