- Top
- Maintenance
- Warning system
- Cases indicated by error codes

# Cases indicated by error codes

Error code | Display | Description | Behavior and cause
--- | --- | --- | ---
[E-30] | [TURN POWER OFF] [P2 CARD] | An error occurred in the camera built-in memory because the P2 card being accessed was ejected. Tally lamp flashes four times per second. | Cannot operate. Follow the message to turn off the power once and turn on the power again. Ensure that there is no error in the clips on the ejected card, and restore the clips as necessary.
[E-31] | [TURN POWER OFF] [SYSTEM MODE] | System mode error occurred. Tally lamp flashes four times per second. | Cannot operate. Follow the message to turn off the power once, turn on the power again, and check that there is no error display.
[E-33] | [SYSTEM ERROR] [CAMERA] | Camera unit error occurred. Tally lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-35] | [SYSTEM ERROR] [CODEC] | Codec control error occurred. Tally lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-36] | [SYSTEM ERROR] [P2 SYSTEM] | P2 system error occurred. Tally lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-37] | [SYSTEM ERROR] [P2CS] | P2CS microcomputer error occurred. Tally lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-39] | [SYSTEM ERROR] [INITIALIZE] | Video initialization error occurred. Tally lamp flashes four times per second. | The operation stops. Contact your dealer.
[E-64] | [SYSTEM ERROR] [FRAME SIGNAL] (or no display) | Reference signal error occurred. Tally lamp flashes four times per second. | The operation stops. Contact your dealer.

Top of the page