- Top
- Menu Operations
- Setting menu structure
- Main menu structure

# Main menu structure

[SCENE FILE] | Configures the settings for scene files. This item is used to configure detailed image quality settings of the camera images, to select scene files, and to configure the settings for reading/writing of scene file data to the internal memory. This menu item cannot be set when the thumbnail screen is displayed.
[SYSTEM MODE] | Configures the settings for the recording format of video and audio.
[USER SW] | Sets the functions to be assigned to the USER buttons (USER1 to USER8).
[SW MODE] | Configures the operations of each mode when switched the mode using each switch. This menu item cannot be set when the thumbnail screen is displayed.
[AUTO SW] | Configures the settings for the auto mode. Auto iris, auto gain control, auto tracking white balance, and auto focus functions can be set separately. This menu item cannot be set when the thumbnail screen is displayed.
[RECORDING SETUP] | Configures various settings when performing recording and playback. Set the system frequency, the number of lines, recording format, and recording method.
[CLIP] | Used when performing various tasks, such as playing back, deleting, and copying clips, and editing metadata, while checking the thumbnail of the clips displayed in the viewfinder or LCD monitor. This menu item is enabled when the thumbnail screen is displayed. Clip operations such as [DELETE] or [COPY] are enabled when the target thumbnail is selected. Some items are displayed only in specific situations such as in USB host mode or on the explorer screen.
[AUDIO SETUP] | Configures the settings for audio input/output.
[OUTPUT SEL] | Configures the settings for video output from the <SDI OUT>, <HDMI OUT>, <GENLOCK IN/VIDEO OUT>, and <TC IN/OUT> terminals.
[NETWORK SETUP] | Configures the settings for network.
[DISPLAY SETUP] | Configures the settings for the details to be displayed in the viewfinder or LCD monitor. This menu item cannot be set when the thumbnail screen is displayed.
[CARD FUNCTIONS] | Configures the settings for reading/writing of scene files and user files to SD memory cards.
[OTHER FUNCTIONS] | Configures the settings for reading/writing of user files to internal memory and initialization, and the camera settings.
[MAINTENANCE] | Used for performing maintenance of the camera. This item is used when updating the firmware version of the camera.
[DIAGNOSTIC] | Displays the firmware version, product name, serial number, and energized time of the camera.
[USER MENU SEL] | Sets the items to be displayed in [USER MENU].

Top of the page