- Top
- Shooting
- Variable frame rate (VFR) recording function
- Standard variable frame rate recording (pull-down recording)

# Standard variable frame rate recording (pull-down recording)

Set [1080-59.94P] ([1080-50P]) in the main menu → [SYSTEM MODE] → [LINE&FREQ].

Set [AVC-I100/60P] or [AVC-I100/50P] in the main menu → [SYSTEM MODE] → [REC FORMAT].

Set [ON] in the main menu → [SCENE FILE] → [VFR].

Set the frame rate according to the shooting conditions in the main menu → [SCENE FILE] → [FRAME RATE].

[FRAME RATE] can be changed using the <SEL/PUSH SET> dial button. For details, refer to “Direct menu operation”.

Press the recording button.

Recording starts in standard variable frame rate.

NOTE

- During standard variable frame rate recording, pre-recording, loop recording, interval recording, one-shot recording, dual codec recording, and one-clip recording can not be performed.

- Audio can be recorded.

- Auto iris, auto focus, and auto tracking white balance do not function when the frame rate is set to [9fps] or lower, or when the shutter speed is set to lower than 1/12. They must be operated manually.

Top of the page