- Top
- Shooting
- Setting the high dynamic range (HDR)
- Recording to the external input signal of high dynamic range (HDR)

# Recording to the external input signal of high dynamic range (HDR)

Detects the high dynamic range information of the external input signal and sets as follows.

#### When the high dynamic range information is the high dynamic range

- External input signal is recorded directly in high dynamic range (hybrid log gamma).

- <SDI OUT1> terminal: External input signal is output directly in high dynamic range (hybrid log gamma).

- <SDI OUT2> terminal: When the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT2 HDR] is set to [ON], external input signal is output directly in high dynamic range (hybrid log gamma).

  When the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT2 HDR] is set to [OFF], the external input signal is converted to standard dynamic range (monitoring gamma) for output.

  When changing the setting of [SDI OUT2 HDR], set the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL] to [HLG].

- <HDMI OUT> terminal, <VIDEO OUT> terminal, viewfinder and LCD monitor: Converts an external input signal to the monitoring gamma for output.

- [HLG] is displayed for the gamma mode display on the viewfinder and LCD monitor screen.

#### When the high dynamic range information is the standard dynamic range or there is no high dynamic range information

- External input signal is directly recorded.

  High dynamic range information is recorded as standard dynamic range.

- <SDI OUT1> terminal, <SDI OUT2> terminal, <HDMI OUT> terminal, <VIDEO OUT> terminal, viewfinder, LCD monitor: Outputs external input signal directly.

- Gamma mode display is not displayed on the viewfinder and LCD monitor screen.

NOTE

- Records and outputs in BT.2020 when the color information of the external input signal is BT.2020.

- Recording will continue with information at the start of recording even if the external input signal information is changed during recording.

- The <USER> button to which [VF/LCD HLG] is assigned becomes invalid.

Top of the page