- Top
- Network Connection
- Preparing for connection
- For wireless module other than AJ-WM30/AJ-WM50

# For wireless module other than AJ-WM30/AJ-WM50

Connect the wireless module other than AJ-WM30/AJ-WM50 (optional) to the camera.

Turn off the power of the camera before connecting or disconnecting the wireless module.

<USB2.0> terminal (sub-host)

Fig. 1

Fig. 2

Gap on the cover

Fig. 3

Wireless module

Fig. 4

Fig. 5

Open the cover. (Fig. 1)

Attach the USB 2.0 extension cable to the <USB2.0> terminal (sub-host). (Fig. 2)

Rotate the part at the bottom of the cover in the direction of the arrow (Fig. 3) and close the cover so that the USB 2.0 extension cable goes through the gap. (Fig. 4)

Connect the wireless module. (Fig. 5)

NOTE

- For the USB 2.0 extension cable (optional), using a cable of A type male/female, 0.5 m or shorter, and with double-shielded for noise suppression is recommended.

- For details on wireless modules that can be connected, refer to the support desk at the following website.

  https://pro-av.panasonic.net/en/sales_o/p2/server/4glte.html

  https://pro-av.panasonic.net/en/sales_o/p2/server/wireless_module.html

Top of the page