- Top
- Network Connection
- Network function
- P2 browser function settings and connection status check

# P2 browser function settings and connection status check

## Starting application (P2 Browser) from web browser

After completing the network connection with your mobile device or computer, start the browser of the mobile device or computer, and then start the application (P2 Browser).

Fig. 1

Select [BROWSE] or [BROWSE (+CTRL)] in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [HTTP SERVER].

P2 browser function is enabled.

Start the browser of your mobile device or computer (Safari, Internet Explorer).

Enter the IP address set on the camera in the address entry field of the browser.

- When in the [INFRA] mode and [DHCP] is set to [ENABLE], check the IP address of the camera in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK TOOLS] → [STATUS DISPLAY].

- Factory setting: [192.168.0.1]

If you use a computer, press the Enter key, and if you use iPad/iPhone, tap the GO button.

The web application (P2 Browser) starts up.

Enter [USER NAME] and [PASSWORD] on the entry screen.

Enter [USER NAME] (Factory setting: [guest]) and [PASSWORD] (Factory setting: [p2guest]) of [USER ACCOUNT] that have been set for the camera.

(When a screen like (Fig. 1) appears (for iPad), the connection has been established.

User account name and password can be set in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [USER ACCOUNT].

Accounts can be created or deleted, and the passwords can be changed in the main menu → [I/F SETUP] → [USB/LAN] → [NETWORK FUNC] → [ACCOUNT LIST].

User account name must not exceed 31 characters.The password must be 6 to 15 characters long.

For information on P2 Browser, refer to the “P2 Web Application” User Guide from the following website.

https://pro-av.panasonic.net/manual/en/index.html

NOTE

- When [NETWORK SEL] is [OFF] or [4G/LTE], network functions cannot be used.

## Network operation status display (mode check function)

Push the <MARKER SEL>/<MODE CHECK/MENU CANCEL> switch towards the <MCK/MCL> side three times to check the network operation status in the mode check [FUNCTION] screen.

For details, refer to “[FUNCTION] screen”.

Top of the page