- Top
- Shooting
- Setting the high dynamic range (HDR)

# Setting the high dynamic range (HDR)

The camera can record in hybrid log gamma (HLG) when [1080-59.94P]/[1080-50P]/[1080-59.94i]/[1080-50i]/[1080-23.98PsF]/[720-59.94P]/[720-50P] are selected in the main menu → [SYSTEM] → [SYSTEM MODE] → [LINE&FREQ].

NOTE

- When [HLG] is selected in the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL], the following setting menu cannot be set. [DRS], [Y GET], and [B.GAMMA] assigned to the <USER> button are also disabled.

  - [MASTER GAMMA], [BLACK GAMMA], and [B. GAMMA RANGE] in the main menu → [PAINT] → [LOW SETTING]/[MID SETTING]/[HIGH SETTING]

  - [KNEE APE LVL] in the main menu → [PAINT] → [ADDITIONAL DTL]

  - [[S] MANUAL KNEE], [KNEE MASTER POINT], [KNEE MASTER SLOPE], [[S] WHITE CLIP], [WHITE CLIP LVL], [A.KNEE POINT], [A.KNEE LVL], [A.KNEE RESPONSE], [DRS MODE], [DRS EFFECT DEPTH], [[S] HI-COLOR SW], and [HI-COLOR LVL] in the main menu → [PAINT] → [KNEE/LEVEL]

  - [MASTER GAMMA], [R GAMMA], [B GAMMA], [F-REC DYNAMIC LVL], [F-REC BLACK STR LVL], [V-REC KNEE SLOPE], and [V-REC KNEE POINT] in the main menu → [PAINT] → [GAMMA]

  - [GAMMA] in the main menu → [PAINT] → [[S] CAMERA SETTING]

  - [AUTO KNEE SW] in the main menu → [CAMERA] → [SW MODE]

  - [LOW LIGHT LVL] in the main menu → [VF] → [VF DISPLAY]

  - [COLOR CHECK] in the main menu → [MAINTENANCE] → [SYSTEM CHECK]

- When the main menu → [SYSTEM] → [SYSTEM MODE] → [REC FORMAT] is set to [DVCPRO HD/60P]/[DVCPRO HD/60i]/[DVCPRO HD/50P]/[DVCPRO HD/50i] and a video is recorded with hybrid log gamma, a warning message is displayed for approximately three seconds on the viewfinder and LCD monitor. Information for the hybrid log gamma, BT.709, and BT.2020 cannot be recorded at this time although a video can be recorded.

- A clip with proxy data recorded with the recording format of the proxy data set to AVC-G6 and hybrid log gamma BT.709 cannot be played back in P2 Viewer Plus for Windows.

  Play back using Windows Media Player in Windows or VLC Media Player Ver.2.0 and above.

Recording in high dynamic range (HDR)
Playing back the signal recorded in high dynamic range (HDR)
Recording to the external input signal of high dynamic range (HDR)
Top of the page