- Top
- Shooting
- Handling setting data
- Writing and reading lens files to and from SD memory card

# Writing and reading lens files to and from SD memory card

Eight lens files stored to internal memory on the camera can be written to SD memory card as a card file with a single title. Eight titles can be written to SD memory card. Lens files written to SD memory card can be read to internal memory as a written title (containing eight lens files).

The following shows the relationship between lens files stored to internal memory and lens files written to SD memory card.

Internal memory

8 lens files

Up to eight lens files can be stored in internal memory.

The contents of the eight lens files can be written to and read from SD memory cards as a card file with a single title.

Card file

Title 1

Title 2

Title 3

Title 4

Eight lens files×8 = 64 lens files can be written.

Title 5

Title 6

Title 7

Title 8

## Writing lens files to SD memory card

Fig. 1

Fig. 2

Select [SAVE] in the main menu → [FILE] → [LENS FILE (SD CARD)], and press the jog dial button (or <SET> button). (Fig. 1)

The list of lens files currently saved in camera memory is displayed.

Select the file to write from the file list. (Fig. 2)

The title entry screen and keyboard are displayed.

Enter the desired characters with the keyboard.

Use the jog dial button (or cursor buttons ///) to select [OK], and press the jog dial button (or <SET> button).

The confirmation screen is displayed.

Select [YES], and press the jog dial button (or <SET> button).

The file is saved and the file list is updated.

For details on error messages if an error message is displayed, refer to “Warning/error displays in the thumbnail operation, menu operation, and USB storage mode”.

## Reading lens files from SD memory card

Select [LOAD] in the main menu → [FILE] → [LENS FILE (SD CARD)], and press the jog dial button (or <SET> button).

The list of lens files currently saved in camera memory is displayed.

Select the file name to read, and press the jog dial button (or <SET> button).

The confirmation screen is displayed.

Select [YES], and press the jog dial button (or <SET> button).

Loading of the file begins.

When the completion message is displayed, press the jog dial button (or <SET> button).

For details on error messages if an error message is displayed, refer to “Warning/error displays in the thumbnail operation, menu operation, and USB storage mode”.

NOTE

- Titles of card files on SD memory cards are displayed on the [LENS FILE (SD CARD)] screen. However, titles of lens files contained inside card files are not displayed on the [LENS FILE (SD CARD)] screen. Read the files and check on the [LENS FILE] screen, whenever required. At this time, the lens file in internal memory will be rewritten with the lens file that is read. Before reading lens files on SD memory cards, write the lens files in internal memory to SD memory card to make a backup.

## CAC file

For details, refer to “Chromatic aberration compensation function (CAC)”.

Top of the page