- Top
- Menu Operations
- Menu list
- [I/F SETUP]

# [I/F SETUP]

These are items for setting related to audio and video input/output and display, and setting battery, audio, video output, etc.

## [OUTPUT SEL]

Item | Description of settings
--- | ---
[OUTPUT ITEM] | Sets the character content to superimpose on the output signal of the <SDI OUT1> terminal and monitor output terminal (<SDI OUT2>, <HDMI OUT>, and <VIDEO OUT>). [MENU ONLY]: Displays only on the menu. Normally, nothing is displayed. [TC]: Displays the time code. (Menu is displayed on the menu) [STATUS]: Displays all items that are the same as the characters displayed on the viewfinder. (Menu is displayed on the menu) Factory setting: [MENU ONLY] The time code display position moves up and down based on the camera ID position.
[SDI OUT1] | Turns <SDI OUT1> terminal output [ON]/[OFF]. [ON]: Performs output. [OFF]: Stops output. Factory setting: [ON]
[SDI OUT1 MODE] | Selects <SDI OUT1> terminal output signals. [MEM]: In playback mode, these are playback images. [CAM]: When the main menu → [SYSTEM] → [SYSTEM MODE] → [REC SIGNAL] is set to [CAM], output is always camera images. Factory setting: [MEM]
[SDI OUT1 CHAR] | Selects whether to superimpose characters on <SDI OUT1> terminal output images. [ON]: Superimposes. [OFF]: Does not superimpose. Factory setting: [OFF] The content of characters to superimpose is the same as the characters superimposed on images output from <SDI OUT2> and other terminals.
[SDI OUT2] | Turns <SDI OUT2> terminal output [ON]/[OFF]. [ON]: Performs output. [OFF]: Stops output. Factory setting: [OFF]
[SDI OUT2 HDR] | Select high dynamic range/standard dynamic rage for the output of <SDI OUT2> terminal. [ON]: Outputs in high dynamic range. [OFF]: Outputs in standard dynamic range. This is only enabled when the main menu → [PAINT] → [GAMMA] → [GAMMA MODE SEL] is set to [HLG].
[VIDEO OUT] | Turns <VIDEO OUT> terminal output [ON]/[OFF]. [ON]: Performs output. [OFF]: Stops output. Factory setting: [OFF]
[SDI2/HDMI OUT] | Selects the signal form to be output to the monitor output terminal (<SDI OUT2> or <HDMI OUT>) in HD mode. [SYSTEM MODE]: Outputs in the system mode signal format. [DOWNCON]: Outputs the down converter signal. Factory setting: [SYSTEM MODE]
[1080P SDI2/HDMI OUT] | Selects whether to convert the output signal of the monitor output terminal (<SDI OUT2> or <HDMI OUT>) to 1080i when in 1080P mode. [1080P]: Outputs as 1080P. [1080i]: Converts to 1080i and outputs. Factory setting: [1080P] If the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI2/HDMI OUT] is set to [DOWNCON], the signal that was down-converted is output, regardless of these settings.
[3G-SDI OUT] | Selects 1080P signals of the HD SDI output in 1080P mode. [LEVEL-A]: Selects the LEVEL-A method. [LEVEL-B]: Selects the LEVEL-B DL method. Factory setting: [LEVEL-B]
[MONITOR OUT MODE] | Selects the output signals of the monitor output terminal (<SDI OUT2>, <HDMI OUT> or <VIDEO OUT2>). Operates independently of the <SDI OUT1> terminal. [MEM]: In playback mode, these are playback images. [CAM]: When the main menu → [SYSTEM] → [SYSTEM MODE] → [REC SIGNAL] is set to [CAM], output is always camera images. Factory setting: [MEM]
[MONITOR OUT ZEBRA] | Selects whether the zebra pattern is superimposed over the output video signals from the monitor output terminals (<SDI OUT2>, <HDMI OUT>, and <VIDEO OUT>). (The remote VBS signal also interlocks.) [ON]: Superimposes. [OFF]: Does not superimpose. Factory setting: [OFF]
[SDI EDH] | Sets whether to add an error detection flag to SD SDI output. [ON], [OFF] Factory setting: [ON]
[HDSDI REMOTE] | Sets whether to use the control function of recording operation for an external device (such as a recorder) connected to the <SDI OUT1> terminal or <SDI OUT2> terminal. (At HD SDI output) [ON], [OFF] Factory setting: [OFF] Selecting [ON] outputs recording operation control to an external device. While recording is instructed, the red tally lamp, front tally lamp, back tally lamp of the viewfinder of the camera, and the rear tally lamp of the camera illuminate. The display method for the recording status of the camera can be selected from the main menu → [REC/PB] → [REC/PB SETUP] → [REC TALLY]. Recording operation control is not output in interval recording, one-shot recording, and loop recording. Recording operation control is not output when 4G/LTE is set.
[THUMBNAIL OUT] | Selects whether to output the thumbnail of a clip displayed on the LCD monitor to the <SDI OUT1> terminal, <SDI OUT2> terminal, <HDMI OUT> terminal, and <VIDEO OUT> terminal. [ON]: Performs output. [OFF]: Does not output. Factory setting: [OFF]

## [SDI OUT1 MARKER]

Item | Description of settings
--- | ---
[MARKER SW] | Switches the marker. [ON]: Displays. [OFF]: Does not display. Factory setting: [OFF]
[CENTER MARK] | Switches the center marker. [1]:+(large) [2]: Open center (large) [3]:+(small) [4]: Open center (small) [OFF]: Does not display. Factory setting: [1]
[SAFETY MARK] | Selects the type of frame for the safety zone marker. [1]: Box [2]: Corners [OFF]: Does not display. Factory setting: [2]
[SAFETY AREA] | Sets the size of the safety zone marker. The constant ratio of length to width can be set in 1% increments. [80%]…[100%] Factory setting: [90%]
[FRAME MARK] | Enables/disables frame marker. [ON], [OFF] Factory setting: [OFF]
[FRAME SIG] | Sets frame marker aspect ratio. [4:3], [13:9], [14:9], [VISTA], [CNSCO] Factory setting: [4:3] [VISTA] is 16:8.65, and [CNSCO] is 16:6.81.
[USER BOX] | Sets whether to display the user box to the signal from the <SDI OUT1> terminal. [ON], [OFF] Factory setting: [OFF]
[USER BOX WIDTH] | Sets the width of the user box. [1]…[100] Factory setting: [13]
[USER BOX HEIGHT] | Sets the height of the user box. [1]…[100] Factory setting: [13]
[USER BOX H POS] | Sets the horizontal position of the center of the user box. [−50]…[50] Factory setting: [0]
[USER BOX V POS] | Sets the vertical position of the center of the user box. [−50]…[50] Factory setting: [0]

## [MONI OUT MARKER]

Item | Description of settings
--- | ---
[CENTER MARK] | Switches the center marker. [1]:+(large) [2]: Open center (large) [3]: +(small) [4]: Open center (small) [OFF]: Does not display. Factory setting: [1]
[SAFETY MARK] | Selects the type of frame for the safety zone marker. [1] Box [2] Corners [OFF] Does not display. Factory setting: [2] If the main menu → [I/F SETUP] → [DOWNCON SETTING] → [DOWNCON MODE] is set to [SIDE CROP] or [LETTER BOX], the safety zone marker is not displayed to the down converter output signal in HD mode.
[SAFETY AREA] | Sets the size of the safety zone marker. The constant ratio of length to width can be set in 1% increments. [80%]…[100%] Factory setting: [90%]
[FRAME MARK] | Enables/disables frame marker. [ON], [OFF] Factory setting: [OFF]
[FRAME SIG] | Sets frame marker aspect ratio. [4:3], [13:9], [14:9], [VISTA], [CNSCO] Factory setting: [4:3] [VISTA] is 16:8.65, and [CNSCO] is 16:6.81.
[USER BOX] | Sets whether to display the user box to the signal from the monitor output terminal (<SDI OUT2>, <HDMI OUT>, or <VIDEO OUT>). [ON], [OFF] Factory setting: [OFF] If the main menu → [I/F SETUP] → [DOWNCON SETTING] → [DOWNCON MODE] is set to [SIDE CROP] or [LETTER BOX], the user box is not displayed to the down converter output signal in HD mode.
[USER BOX WIDTH] | Sets the width of the user box. [1]…[100] Factory setting: [13]
[USER BOX HEIGHT] | Sets the height of the user box. [1]…[100] Factory setting: [13]
[USER BOX H POS] | Sets the horizontal position of the center of the user box. [−50]…[50] Factory setting: [0]
[USER BOX V POS] | Sets the vertical position of the center of the user box. [−50]…[50] Factory setting: [0]

## [DOWNCON SETTING]

Item | Description of settings
--- | ---
[DOWNCON MODE] | Sets the mode of the down converter output signal. [SIDE CROP], [LETTER BOX], [SQUEEZE] Factory setting: [SQUEEZE] When [LETTER BOX] is selected, some parts of the top and bottom edges of the down converter output video may be distorted. This is not a malfunction.
[DETAIL] | Turns detail function for the down converter output signal [ON]/[OFF]. The down converter output signal contains detail components set during HD signal processing. This setting superimposes the detail components exclusive to down converter output to that signal. [ON], [OFF] Factory setting: [ON] Even if this setting is [OFF], the detail components set during HD signal processing cannot be disabled.
[H.DTL LEVEL] | Sets horizontal detail correction level for the down converter output signal. [0]…[31] Factory setting: [8]
[V.DTL LEVEL] | Sets vertical detail correction level for the down converter output signal. [0]…[31] Factory setting: [4]
[DTL CORING] | Sets the detail noise removal level. [0]…[15] Factory setting: [1]
[H.DTL FREQ.] | Selects the horizontal detail frequency. [2.5MHz], [3MHz], [3.5MHz], [4MHz], [4.5MHz] Factory setting: [3.5MHz]
[2D LPF] | Sets the filter. [ON]: Reduces cross colors. [OFF]: Does not reduce cross colors. Factory setting: [OFF]

## [GENLOCK]

Item | Description of settings
--- | ---
[GENLOCK] | Switches the synchronization signal of the camera signal. [INT]: Synchronizes to the internal standard signal independent of standard signals input to the <GENLOCK IN> terminal or <SDI IN> terminal. [GL IN]: Synchronizes to the standard signal input to the <GENLOCK IN> terminal. [SDI IN]: Synchronizes to the standard signal input to the <SDI IN> terminal. Factory setting: [INT] When the main menu → [SYSTEM] → [SYSTEM MODE] → [REC SIGNAL] is set to [SDI], the camera synchronizes to the reference signal input to the <SDI IN> terminal regardless of this setting.
[GL PHASE] | Selects the output signal of phase to be locked to the signal input to the <GENLOCK IN> terminal. [HD SDI]: Locks the HD SDI output signal to genlock input. The video start position of the down converter output signal lags by approx. 90 lines. [COMPOSITE]: Locks the down converter output signal to genlock input. The video start position of the HD SDI output signal advances by approx. 90 lines. Factory setting: [HD SDI] This item is not displayed in SD mode (480/59.94i and 576/50i).
[H PHASE COARSE] | Roughly adjusts to match horizontal synchronization phase when building a system. [−100]…[100] Factory setting: [0]
[H PHASE FINE] | Minutely adjusts to match horizontal synchronization phase when building a system. [−100]…[100] Factory setting: [0]

## [MIC/AUDIO]

Item | Description of settings
--- | ---
[VR SELECT] | Selects which channel to assign to the <AUDIO LEVEL CH1/3>/<AUDIO LEVEL CH2/4> and <F.AUDIO LEVEL> dials. [CH1/2]: Assigns level adjustment of channels 1/2. Channels 3/4 can be automatically adjusted or adjusted by [LVL CONTROL CH3] or [LVL CONTROL CH4]. [CH3/4]: Assigns level adjustment of channels 3/4. Channels 1/2 can be automatically adjusted or adjusted by [LVL CONTROL CH1] or [LVL CONTROL CH2]. Factory setting: [CH1/2] When [CH3/4] is selected in [VR SELECT], channels are also replaced for the following six items. [FRONT VR CH1] → [FRONT VR CH3] [FRONT VR CH2] → [FRONT VR CH4] [AUTO LVL CH3] → [AUTO LVL CH1] [AUTO LVL CH4] → [AUTO LVL CH2] [LVL CONTROL CH3] → [LVL CONTROL CH1] [LVL CONTROL CH4] → [LVL CONTROL CH2] For details, refer to “Adjusting the recording levels”.
[FRONT VR CH1(CH3)] | Sets whether to enable the <F.AUDIO LEVEL> dial for input signals selected in audio CH1 (CH3). [FRONT]: Enabled only when [FRONT] is selected. [W.L.]: Enabled only when wireless microphone receiver is selected. [REAR]: Enabled only when [REAR] is selected. [ALL]: Enabled when any input is selected. [OFF]: Disabled regardless of the input selected. Recording levels do not change even if the volume dial is turned. Factory setting: [OFF] The channel is replaced when [CH3/4] is selected in [VR SELECT]. Setting values are inherited between replaced channels.
[FRONT VR CH2(CH4)] | Sets whether to enable the <F.AUDIO LEVEL> dial for input signals selected in audio CH2 (CH4). [FRONT]: Enabled only when [FRONT] is selected. [W.L.]: Enabled only when wireless microphone receiver is selected. [REAR]: Enabled only when [REAR] is selected. [ALL]: Enabled when any input is selected. [OFF]: Disabled regardless of the input selected. Recording levels do not change even if the volume dial is turned. Factory setting: [OFF] The channel is replaced when [CH3/4] is selected in [VR SELECT]. Setting values are inherited between replaced channels.
[AUTO LVL CH3(CH1)] | Selects whether to automatically adjust the level adjustment method for audio CH3 (CH1). [ON]: Automatic adjustment is enabled. [OFF]: Automatic adjustment is disabled. Can be adjusted using [LVL CONTROL CH3(CH1)] at this time. Factory setting: [ON] The channel is replaced when [CH3/4] is selected in [VR SELECT]. Setting values are inherited between replaced channels.
[AUTO LVL CH4(CH2)] | Selects whether to automatically adjust the level adjustment method for audio CH4 (CH2). [ON]: Automatic adjustment is enabled. [OFF]: Automatic adjustment is disabled. Can be adjusted using [LVL CONTROL CH4(CH2)] at this time. Factory setting: [ON] The channel is replaced when [CH3/4] is selected in [VR SELECT]. Setting values are inherited between replaced channels.
[LVL CONTROL CH3(CH1)] | Can be manually adjusted with this item when automatic level adjustment of audio CH3 (CH1) is [OFF]. [0]…[100] Factory setting: [70] The channel is replaced when [CH3/4] is selected in [VR SELECT]. Setting values are inherited between replaced channels.
[LVL CONTROL CH4(CH2)] | Can be manually adjusted with this item when automatic level adjustment of audio CH4 (CH2) is [OFF]. [0]…[100] Factory setting: [70] The channel is replaced when [CH3/4] is selected in [VR SELECT]. Setting values are inherited between replaced channels.
[MIC LOWCUT CH1] | Selects the microphone lowcut filter for input channel 1. [FRONT]: Works when the front microphone is selected. [W.L.]: Enabled only when wireless microphone receiver is selected. [REAR]: Enabled only when the rear microphone is selected. [OFF]: The microphone lowcut filter does not work for any input. Factory setting: [OFF]
[MIC LOWCUT CH2] | Selects the microphone lowcut filter for input channel 2. [FRONT]: Works when the front microphone is selected. [W.L.]: Enabled only when wireless microphone receiver is selected. [REAR]: Enabled only when the rear microphone is selected. [OFF]: The microphone lowcut filter does not work for any input. Factory setting: [OFF]
[MIC LOWCUT CH3] | Selects the microphone lowcut filter for input channel 3. [FRONT]: Works when the front microphone is selected. [W.L.]: Enabled only when wireless microphone receiver is selected. [REAR]: Enabled only when the rear microphone is selected. [OFF]: The microphone lowcut filter does not work for any input. Factory setting: [OFF]
[MIC LOWCUT CH4] | Selects the microphone lowcut filter for input channel 4. [FRONT]: Works when the front microphone is selected. [W.L.]: Enabled only when wireless microphone receiver is selected. [REAR]: Enabled only when the rear microphone is selected. [OFF]: The microphone lowcut filter does not work for any input. Factory setting: [OFF]
[LIMITER CH1] | Selects the channel 1 limiter. Disabled when automatic adjustment of recording levels is selected. [ON], [OFF] Factory setting: [OFF]
[LIMITER CH2] | Selects the channel 2 limiter. Disabled when automatic adjustment of recording levels is selected. [ON], [OFF] Factory setting: [OFF]
[LIMITER CH3] | Selects the channel 3 limiter. Disabled when automatic adjustment of recording levels is selected. [ON], [OFF] Factory setting: [OFF]
[LIMITER CH4] | Selects the channel 4 limiter. Disabled when automatic adjustment of recording levels is selected. [ON], [OFF] Factory setting: [OFF]
[TEST TONE] | Selects test signals. [NORMAL]: Outputs test tones to all channels if the <OUTPUT> switch is <BARS>, and <CH1> on the <AUDIO IN> switch is set to <FRONT>. [ALWAYS]: Outputs test tones to all channels at all times when the <OUTPUT> switch is <BARS>. [CHSEL]: When the <OUTPUT> switch is <BARS>, outputs test tones to the channel for which <CH1> or <CH2> on the <AUDIO IN> switch is set to <FRONT>. The test tones are not output to CH3 and CH4. [OFF]: Does not output the test tone. Factory setting: [NORMAL]
[FRONT MIC POWER] | Sets the phantom power of the front microphone. [ON], [OFF] Factory setting: [ON]
[REAR MIC POWER] | Sets the phantom power of the rear microphone. Phantom power is not output when [OFF] is selected, even if the <REAR AUDIO CH1> and <REAR AUDIO CH2> switches are set to <+48V>. [ON], [OFF] Factory setting: [ON]
[MONITOR SELECT] | Selects the signal method to output to the monitor when the <MONITOR SELECT> switch is set to <ST> (stereo). [STEREO], [MIX] Factory setting: [STEREO]
[FRONT MIC LEVEL] | Selects the front microphone input level. [−40dB], [−50dB] Factory setting: [−40dB]
[REAR MIC CH1/3 LVL] | Selects the rear microphone input level. [−50dB], [−60dB] Factory setting: [−60dB]
[REAR MIC CH2/4 LVL] | Selects the rear microphone input level. [−50dB], [−60dB] Factory setting: [−60dB]
[REAR LINE IN LVL] | Selects the rear line input level. [−3dB], [0dB], [4dB] Factory setting: [4dB]
[AUDIO OUT LVL] | Selects the audio output level. [−3dB], [0dB], [4dB] Factory setting: [4dB]
[HEADROOM] | Sets the headroom (standard level). [18dB], [20dB] Factory setting: [20dB]
[WIRELESS WARN] | Sets whether to display a warning when the reception status of the wireless microphone receiver is poor. [ON], [OFF] Factory setting: [OFF]
[WIRELESS TYPE] | Selects the type of wireless microphone receiver. [SINGLE]: Selects a single channel type wireless microphone receiver. [DUAL]: Selects a double channel type wireless microphone receiver. Factory setting: [SINGLE]

## [USB/LAN]

[4G/LTE PROPERTY] cannot be selected when the setting is not required on the connected 4G/LTE USB modem.

Item | Description of settings
--- | ---
[USB MODE SELECT] | Sets the camera operation mode when an external device is connected to the USB. [STORAGE]: Sets the mode to be used with connected devices such as an external hard disk drive. [DEVICE]: Selects the USB device mode for using P2 cards as mass storage, using computers or other devices connected via USB 2.0. Factory setting: [STORAGE] This item cannot be changed when [USB MODE] is set to [ON].
[USB MODE] | Turns operation of the mode selected in [USB MODE SELECT] [ON]/[OFF]. [ON], [OFF] Factory setting: [OFF] Once the power is turned off, it is always set to [OFF] the next time power is turned on. When [DEVICE] is selected for [USB MODE SELECT] and [USB MODE] is set to [ON] (in USB device mode), the menu cannot be opened. In this case, you can exit the USB device mode (return to [OFF]) by pressing the <EXIT> mode. For details, refer to “Connecting to a computer in the USB device mode”. The setting cannot be changed while the thumbnail screen is displayed.
[NETWORK SEL] | Sets the connection method when connecting the camera with an external device (such as a computer) via network. [WLAN]: Connects via wireless LAN. [4G/LTE]: Connects via 3G/4G/LTE. [LAN]: Connects via the <LAN> terminal. [OFF]: Does not connect. Factory setting: [OFF]
[NETWORK FUNC] | [HTTP SERVER] | Configures the settings regarding the HTTP server function. [BROWSE]: Enables the P2 browser function. [BROWSE (+CTRL)]: Enables the HTTP server function, starting and stopping recording at the terminal side, and preset control of time code or user bits. [DISABLE]: Disables the HTTP server function. Factory setting: [DISABLE]
| [PLAYLIST] | Sets entering/exiting of the playlist edit mode. [ON], [OFF] Factory setting: [OFF]
| [IP REMOTE] | [ENABLE]: Enables remote control with IP connection. [DISABLE]: Disables remote control with IP connection. Factory setting: [DISABLE] Some functions can be remote controlled from the remote operation panel AK-HRP200G (optional) connected via IP. For details, refer to “Connecting to Remote operation panel (AK-HRP200G)”. When [ENABLE] is selected, remote control from the extension control unit (AG-EC4G) or the remote operation panel AK-HRP200G (optional) connected to the <REMOTE> terminal is disabled.
| [USER ACCOUNT] | Sets the user account name.
| [ACCOUNT LIST] | Displays the currently set account name. Registering of new accounts, deleting accounts, or changing password can also be performed.
[FTP CLIENT SERVICE] | [SETTING DATA] | Sets the source from where client service settings are acquired. [INTERNAL]: Uses the settings set on the camera. [SD CARD]: Uses the settings of the file inside the SD memory card inserted in the SD card slot. When this item is set to [SD CARD], insert an SD memory card before turning on the power of the camera. Factory setting: [INTERNAL]
| [SERVER URL] | Sets the name or address of the destination server.
| [LOGIN USER] | Sets the login user ID.
| [LOGIN PASSWORD] | Sets the login password.
| [SSH] | Sets when transferring files using SSH. [ENABLE]: Uses SSH. [DISABLE]: Does not use SSH. Factory setting: [DISABLE]
| [SSH PORT] | Sets the network port number when SSH is used. Set to the same number as the server. The menu setting value is displayed with []. Factory setting: [22]
| [LOAD (SD CARD)] | Loads the settings of the client service from the SD memory card.
| [SAVE (SD CARD)] | Saves the settings of the client service onto the SD memory card.
| [REC DURING UPLOAD] | Sets whether to use the rec during upload function. [ENABLE]: Uses the rec during upload function. [DISABLE]: Does not use the rec during upload function. Factory setting: [DISABLE]
| [AUTO UPLOAD] | Sets whether to enable the function to register clips recorded using the camera automatically to the upload list when recording stops, and if enabled, sets the type of target clip. [REC CLIP(PROXY)]: Upload target is proxy data of recorded clips. [REC CLIP]: Upload target is recorded clips (main recording data and proxy data). [DISABLE]: Recorded clips are not upload targets. Factory setting: [DISABLE]
| [UPLOAD LIST] | Displays the list information of clips to upload.
| [SAVE LOG (SD CARD)] | Save up to the latest 1000 logs for clip information (month and date, clip number (global clip ID), status) registered in the upload list to an SD memory card.
[STREAMING SETTING] | [START TRIGGER] | Sets the method for starting video streaming. [CAMERA]: Starts/stops streaming from the camera. [RECEIVER]: Operates the start/stop of the streaming distribution from the terminal on the network using the P2 Browser or the P2 Streaming Receiver. Factory setting: [RECEIVER]
| [SETTING DATA] | Sets the source from where settings for streaming is acquired when [CAMERA] is selected in [START TRIGGER]. [INTERNAL]: Uses the settings set on the camera. [SD CARD]: Uses the settings of the file inside the SD memory card inserted in the SD card slot. When this item is set to [SD CARD], insert an SD memory card before turning on the power of the camera. Factory setting: [INTERNAL]
| [SERVER ADDR.] | Sets the IP address of the device receiving the streaming video when [CAMERA] is selected in [START TRIGGER].
| [RTSP PORT] | Sets the RTSP port number required for streaming when [CAMERA] is selected in [START TRIGGER]. Factory setting: [554]
| [LOAD (SD CARD)] | When [CAMERA] is selected in [START TRIGGER] and [INTERNAL] is selected in [SETTING DATA], the connection information necessary for streaming distribution is read from the SD memory card.
| [SAVE (SD CARD)] | When [CAMERA] is selected in [START TRIGGER] and [INTERNAL] is selected in [SETTING DATA], the connection information necessary for streaming distribution is saved to the SD memory card.
| [START] | When [CAMERA] is selected in [START TRIGGER], the streaming distribution is started/stopped from the camera. [ON]: Starts streaming. [OFF]: Stops streaming.
[LAN PROPERTY] | [MAC ADDRESS] | Displays the MAC address of the <LAN> terminal on the camera. (Cannot be changed.)
| [DHCP] | Sets whether to use automatic acquisition via DHCP. (Mutually exclusive with [DHCP SERVER] setting) [ENABLE]: Uses automatic acquisition. [DISABLE]: Does not use automatic acquisition. Set [IP ADDRESS], [SUBNET MASK], [DEFAULT GATEWAY], [PRIMARY DNS], and [SECONDARY DNS]. Factory setting: [ENABLE]
| [IP ADDRESS] | Sets the IP address when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.1]
| [SUBNET MASK] | Sets the subnet mask when [DISABLE] is selected in [DHCP]. Factory setting: [255.255.255.0]
| [DEFAULT GATEWAY] | Sets the default gateway when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.254]
| [PRIMARY DNS] | Sets the primary DNS server when [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [SECONDARY DNS] | Sets the secondary DNS server when [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [DHCP SERVER] | Sets whether to use the DHCP SERVER function when connected via wired LAN. (Mutually exclusive with [DHCP] setting) [ENABLE]: Uses the DHCP SERVER function. [DISABLE]: Does not use the DHCP SERVER function. Factory setting: [DISABLE]
[WIRELESS PROPERTY] | [MAC ADDRESS] | Displays the MAC address of the wireless LAN of the camera. (Cannot be changed.)
| [TYPE] | Sets the connection method. [DIRECT]: Accesses to the network function of the camera directly from a smartphone, tablet, or computer. [INFRA]: Connects to the wireless access point. Factory setting: [DIRECT]
| [SSID INPUT MODE] | Sets the setting method of SSID. When [TYPE] in [WIRELESS PROPERTY] is set to [INFRA], this item can be set. [SELECT]: Selects from the access point list. [MANUAL]: For entering the access point manually. Factory setting: [SELECT]
| [SSID] | Displays network name (SSID). Factory setting: [AJ-PX5100G]
| [BAND] | Switches between two transmission methods (2.4 GHz or 5 GHz). [2.4GHz], [5GHz] Factory setting: [2.4GHz]
| [CHANNEL (2.4GHz)] | Sets the channels to be used when [DIRECT] is selected in [TYPE], [2.4GHz] is selected in [BAND], and the camera is connected via wireless LAN. [AUTO], [CH1], [CH6], [CH11] Factory setting: [AUTO]
| [CHANNEL (5GHz)] | Sets the channels to be used when [DIRECT] is selected in [TYPE], [5GHz] is selected in [BAND], and the camera is connected via wireless LAN. The selections change according to the wireless module to mount. [AUTO], [CH36], [CH40], [CH44], [CH48], [CH149], [CH153], [CH157], [CH161], [CH165] Factory setting: [AUTO]
| [ENCRYPTION] | Sets the encryption format. [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE] Factory setting: [WPA2-AES]
| [ENCRYPT KEY] | Sets the encryption key. Set the key using a string of 8 to 63 characters or a hexadecimal number with 64 digits. Factory setting: [01234567890123456789abcdef]
| [DHCP] | Sets whether to use automatic acquisition via DHCP when [INFRA] is selected in [TYPE]. [ENABLE]: Uses automatic acquisition. [DISABLE]: Does not use automatic acquisition. Factory setting: [ENABLE]
| [IP ADDRESS] | Sets the IP address when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.1]
| [SUBNET MASK] | Sets the subnet mask when [DISABLE] is selected in [DHCP]. Factory setting: [255.255.255.0]
| [DEFAULT GATEWAY] | Sets the default gateway when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.254]
| [PRIMARY DNS] | Sets the primary DNS server when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [SECONDARY DNS] | Sets the secondary DNS server when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [DHCP SERVER] | Sets whether to use the DHCP SERVER function when [DIRECT] is selected in [TYPE] and the camera is connected via wireless LAN. [ENABLE]: Uses the DHCP SERVER function. [DISABLE]: Does not use the DHCP SERVER function. Factory setting: [ENABLE]
[4G/LTE PROPERTY] | [APN] | Sets the APN (Access Point Name) provided by the provider.
| [USER ID] | Sets the user name provided by the provider.
| [PASSWORD] | Sets the password provided by the provider.
| [DIAL NO.] | Sets the phone number. For details, refer to the manual of the provider you have contracted.
[NETWORK TOOLS] | [LOG DISPLAY] | Displays the connection log.
| [STATUS DISPLAY] | Displays the network status.
| [INITIALIZE] | Restores the network settings to the factory settings.
| [PING] | Checks network connection using PING commands.

## [LCD MONITOR]

Item | Description of settings
--- | ---
[BACKLIGHT] | Adjusts the brightness of the LCD monitor backlight. [−3]: Becomes the darkest. [−2], [−1]: Darkens more than normal. [0]: Normal brightness. [1]: Brightens more than normal. Factory setting: [0]
[BRIGHTNESS] | Adjusts the brightness of the LCD monitor. [−15]…[15] Factory setting: [0]
[COLOR LEVEL] | Adjusts the LCD monitor hue. [−15]…[15] Factory setting: [0]
[CONTRAST] | Adjusts the contrast of the LCD monitor. [−30]…[30] Factory setting: [0]
[SELF SHOOT] | Selects whether to invert the right and left sides of the LCD monitor. [NORMAL]: Does not invert the left and right sides. [MIRROR]: Inverts the left and right sides. Factory setting: [MIRROR]
[VF/LCD CHAR] | Selects whether to display a character on the image of the LCD monitor and viewfinder. [ON]: Displays characters on both the viewfinder and LCD monitor. [VF-OFF]: Does not superimpose on the viewfinder, and displays on the LCD monitor. [LCD-OFF]: Does not superimpose on the LCD monitor, and displays on the viewfinder. Factory setting: [ON] This item can be set in the main menu → [VF] → [VF DISPLAY] as well.

## [BATTERY/P2CARD]

Item | Description of settings
--- | ---
[BATTERY SELECT] | Selects the battery to use. [HYTRON140], [DIONIC90], [ENDURA10], [PAG L96e]: Detects the battery charge level according to the selected battery when Anton/Bauer HYTRON140 or DIONIC90, IDX ENDURA10 (E-10), and PAG PAG L96e are selected. [TYPE A], [TYPE B], [TYPE C]: Select either item when a battery other than [HYTRON140], [DIONIC90], [ENDURA10], and [PAG L96e] is used. At this time, set [FULL] (full voltage), [NEAR END] (near end warning voltage), and [END] (end voltage) in the main menu → [I/F SETUP] → [BATTERY SETTING] according to the battery in use. [BATT STAT]: By selecting [BATT STAT] when using a battery whose charge level is detected as a percentage value, near end and end operations are conducted according to the percentage value of the charge level. Set the percentage value of [BATT STAT NEAR END] (near end) and [BATT STAT END] (end) in the main menu → [I/F SETUP] → [BATTERY SETTING] according to the battery in use. [ENDURA STAT]: Select it when ENDURA battery by IDX is used to perform near end and end operations according to the percentage value of the charge level information. Set the percentage value of [ENDURA STAT NEAR END] (near end) and [ENDURA STAT END] (end) in the main menu → [I/F SETUP] → [BATTERY SETTING] according to the battery in use. Factory setting: [DIONIC90] When the battery charge level percentage cannot be detected, it will follow the setting value of [TYPE A] even if it is set to [BATT STAT] or [ENDURA STAT]. Make sure that the [TYPE A] setting values [FULL] (fully charged), [NEAR END] (near end), or [END] (end) is appropriate for the battery being used.
[EXT DC IN SELECT] | Sets the type of charge level to connect a battery to the <DC IN> terminal. Also detects a charge level that corresponds to the selected type. Information about selecting a battery type is the same as [BATTERY SELECT]. Displays the analog voltage on the viewfinder screen. [DC PWR SUPPLY], [HYTRON140], [DIONIC90], [ENDURA10], [PAG L96e], [TYPE A], [TYPE B], [TYPE C] Factory setting: [DC PWR SUPPLY]
[BATT NEAR END ALARM] | Selects whether to play the warning sound at battery near end. [ON], [OFF] Factory setting: [OFF]
[BATT NEAR END CANCEL] | If set to [ON], the warning sound and warning display output can be canceled when the <MARKER SEL>/<MODE CHECK/MENU CANCEL> switch is pushed towards the <MCK/MCL> side at battery near end. [ON], [OFF] Factory setting: [ON]
[BATT END ALARM] | Sets whether to output the warning sound at battery near end. [ON], [OFF] Factory setting: [ON]
[BATT REMAIN FULL] | Sets the content of the battery remaining charge bar of the status display when a battery with charge level display function is used. [70%]: Displays as full at 70%. [100%]: Displays as full at 100%. Factory setting: [70%]
[CARD NEAR END ALARM] | Sets whether to output the warning sound at P2 card near end. [ON], [OFF] Factory setting: [OFF]
[CARD NEAR END TIME] | Sets remaining time to emit the P2 card near end warning. [2min], [3min] Factory setting: [2min]
[CARD END ALARM] | Sets whether to output the warning sound at P2 card end. [ON], [OFF] Factory setting: [ON]
[CARD REMAIN/Seg] | Sets the time of one segment () for the P2 card remaining capacity bar in the status display. [3min/Seg]: One segment is three minutes [5min/Seg]: One segment is five minutes Factory setting: [3min/Seg]

## [BATTERY SETTING]

Item | Description of settings
--- | ---
[BATTERY MODE] | Selects whether to set the near end voltage of a battery. [AUTO]: Automatically set. [MANUAL]: Manually set. Factory setting: [AUTO]
[HYTRON140 NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [HYTRON140]. [12.0V]…[15.0V] Factory setting: [13.1V] This item is enabled when [BATTERY MODE] is set to [MANUAL].
[DIONIC 90 NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [DIONIC90]. [12.0V]…[15.0V] Factory setting: [13.7V] This item is enabled when [BATTERY MODE] is set to [MANUAL].
[ENDURA10 NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [ENDURA10]. [12.0V]…[15.0V] Factory setting: [13.4V] This item is enabled when [BATTERY MODE] is set to [MANUAL].
[PAG L96e NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [PAG L96e]. [12.0V]…[15.0V] Factory setting: [13.0V] This item is enabled when [BATTERY MODE] is set to [MANUAL].
[TYPE A FULL] | Selects the voltage for full display in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE A]. [13.0V]…[17.0V] Factory setting: [15.6V] The [TYPE A] factory setting corresponds to the IDX ENDURA ELETE.
[TYPE A NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE A]. [11.0V]…[15.0V] Factory setting: [13.2V] The [TYPE A] factory setting corresponds to the IDX ENDURA ELETE.
[TYPE A END] | Selects the end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE A]. [11.0V]…[15.0V] Factory setting: [12.5V] The [TYPE A] factory setting corresponds to the IDX ENDURA ELETE.
[TYPE B FULL] | Selects the voltage for full display in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE B]. [13.0V]…[17.0V] Factory setting: [15.9V] The [TYPE B] factory setting corresponds to the Anton/Bauer DIONIC HC.
[TYPE B NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE B]. [11.0V]…[15.0V] Factory setting: [12.9V] The [TYPE B] factory setting corresponds to the Anton/Bauer DIONIC HC.
[TYPE B END] | Selects the end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE B]. [11.0V]…[15.0V] Factory setting: [12.5V] The [TYPE B] factory setting corresponds to the Anton/Bauer DIONIC HC.
[TYPE C FULL] | Selects the voltage for full display in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE C]. [13.0V]…[17.0V] Factory setting: [15.9V]
[TYPE C NEAR END] | Selects the near end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE C]. [11.0V]…[15.0V] Factory setting: [13.2V]
[TYPE C END] | Selects the end voltage in steps of 0.1 V when the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT] is set to [TYPE C]. [11.0V]…[15.0V] Factory setting: [12.5V]
[BATT STAT NEAR END] | Selects the near end percent value. [4%], [5%], [6%], [7%], [8%], [9%], [10%], [12%], [14%], [16%], [18%], [20%] Factory setting: [5%] When the battery charge level percentage cannot be detected, this will follow the near end voltage value set in [TYPE A]. If a battery is used for which the remaining charge is displayed in units of 10%, the setting value and actual near end warning may vary slightly.
[BATT STAT END] | Selects the end percent value. [1%]…[10%] Factory setting: [1%] When the battery charge level percentage cannot be detected, this will follow the end voltage value set in [TYPE A]. When using a battery which displays battery charge level by units of 10%, end is determined only in two stages: when it is set between [1%] and [5%], or when it is set between [6%] to [10%].
[ENDURA STAT NEAR END] | Selects the near end percent value. [4%], [5%], [6%], [7%], [8%], [9%], [10%], [12%], [14%], [16%], [18%], [20%] Factory setting: [5%] When the battery charge level percentage cannot be detected, this will follow the near end voltage value set in [TYPE A]. If a battery is used for which the remaining charge is displayed in units of 10%, the setting value and actual near end warning may vary slightly.
[ENDURA STAT END] | Selects the end percent value. [1%]…[10%] Factory setting: [1%] When the battery charge level percentage cannot be detected, this will follow the end voltage value set in [TYPE A]. When using a battery which displays battery charge level by units of 10%, end is determined only in two stages: when it is set between [1%] and [5%], or when it is set between [6%] to [10%].

Top of the page