- Top
- Network Connection
- Rec during upload function
- Transferring recorded clips automatically (automatic transfer mode)

# Transferring recorded clips automatically (automatic transfer mode)

Establish the network connection between the camera and a server device.

Refer to “FTP client function setting” for the settings.

Set the camera’s main menu → [I/F SETUP] → [USB/LAN] → [FTP CLIENT SERVICE] → [REC DURING UPLOAD] to [ENABLE].

Select the type of clip to upload in the camera’s main menu → [I/F SETUP] → [USB/LAN] → [FTP CLIENT SERVICE] → [AUTO UPLOAD].

[REC CLIP(PROXY)]: Upload target is proxy data of recorded clips.

[REC CLIP]: Upload target is recorded clips (main recording data and proxy data).

[DISABLE]: Recorded clips are not upload targets.

Shoot.

Clips are registered in the upload list immediately after recording is stopped, and then recorded clips are automatically transferred.

The viewfinder or LCD monitor shows the operation status of the rec during upload function. In addition, the thumbnail screen shows the operation status of the rec during upload function and the transfer status of clips.

NOTE

- Upload of the clip will start after the rec during upload is set to enable. To prevent the upload error, do not remove the card from the P2 memory card slot and the microP2 memory card slot.

- Up to 100 clips can be registered in the upload list for the upload of clips. Clips exceeding 100, excluding the uploaded clips and clips failed to upload cannot be registered.

- While recording is stopped, you can add recorded clips to transfer. From the thumbnail screen, select the main menu → [CLIP] → [COPY] → [FTP] or [FTP(PROXY)], and then select clips to transfer. The selected clips are registered in the upload list.

- Clips are also automatically transferred during recording, playback, and thumbnail display.

- The dividing unit of the recording files will become smaller when [SHORT SPLIT] is selected in the main menu → [REC/PB] → [REC/PB SETUP] → [FILE SPLIT] while the rec during upload function is used, allowing to make the timing to start the clip transfer earlier while recording.

- If the network is disconnected during transfer, or the power of the camera is turned off and on again, transfer resumes in clip units.

- During simultaneous recording, only recorded clips in slot 1 or slot 3 are automatically transferred.

- Clips of interval recording, loop recording, one-clip recording, and one-shot recording are not automatically transferred.

- While the rec during upload function is enabled, the last clip delete function is disabled.

- The directory on the FTP server is not listed in the FTP explorer screen during the transmission or waiting to transmit the clips registered in the upload list.

- While the rec during upload function is enabled, the setting values in the main menu → [I/F SETUP] → [USB/LAN] cannot be changed or initialized.

- The copying between the P2 cards will not operate during the transmission or waiting to transmit the clips registered in the upload list.

- The clip delete function will not operate during the transmission or waiting to transmit the clips registered in the upload list.

- The format function of the P2 card will not operate during the transmission or waiting to transmit the clips registered in the upload list.

Top of the page