- Top
- Network Connection
- Rec during upload function
- Transferring selected clips automatically (manual selection mode)

# Transferring selected clips automatically (manual selection mode)

Fig. 1

Establish the network connection between the camera and a server device.

Refer to “FTP client function setting” for the settings.

Set the camera’s main menu → [I/F SETUP] → [USB/LAN] → [FTP CLIENT SERVICE] → [REC DURING UPLOAD] to [ENABLE].

Set the camera’s main menu → [I/F SETUP] → [USB/LAN] → [FTP CLIENT SERVICE] → [AUTO UPLOAD] to [DISABLE].

From the thumbnail screen, select the main menu → [CLIP] → [COPY] → [FTP] or [FTP(PROXY)], and then select clips to transfer. (Fig. 1)

Selected clips are registered in the upload list, and transferred automatically.

You can check the transfer status of clips registered in the upload list in the main menu → [I/F SETUP] → [USB/LAN] → [FTP CLIENT SERVICE] → [UPLOAD LIST].

The viewfinder or LCD monitor shows the operation status of the rec during upload function. In addition, the thumbnail screen shows the operation status of the rec during upload function and the transfer status of clips.

NOTE

- The clips selected with the manual selection mode will be transferred prioritized to the clips registered to the upload list with the automatic transfer mode.

- Upload of the clip will start after the rec during upload is set to enable. To prevent the upload error, do not remove the card from the P2 memory card slot and the microP2 memory card slot.

- Up to 100 clips can be registered in the upload list for the upload of clips. Clips exceeding 100, excluding the uploaded clips and clips failed to upload cannot be registered.

- Clips are also automatically transferred during recording, playback, and thumbnail display.

- If the network is disconnected during transfer, or the power of the camera is turned off and on again, transfer resumes in clip units.

- While the rec during upload function is enabled, the streaming function is disabled.

- The directory on the FTP server is not listed in the FTP explorer screen during the transmission or waiting to transmit the clips registered in the upload list.

- While the rec during upload function is enabled, the setting values in the main menu → [I/F SETUP] → [USB/LAN] cannot be changed or initialized.

- The copying between the P2 cards will not operate during the transmission or waiting to transmit the clips registered in the upload list.

- The clip delete function will not operate during the transmission or waiting to transmit the clips registered in the upload list.

- The format function of the P2 card will not operate during the transmission or waiting to transmit the clips registered in the upload list.

Top of the page