- Top
- Description of Parts
- Status display
- Memory operation/status related display

# Memory operation/status related display

1. Error code display (Error code)

2. Information display

   [INTERVAL] | Displayed during the interval recording mode.
   [ONE SHOT] | Displayed during the one-shot recording mode.
   [LOOP] | Displayed during the loop recording mode. Flashes when the camera cannot record. (Loop recording)
   [P-REC] | Displayed when the main menu → [REC/PB] → [REC FUNCTION] → [PRE REC] is set to [ON]. [P-REC] flashes when recording is continued after the tally lamp goes out.
   [i-REC] | Displayed during interval recording, and flashes during recording standby.
   [i] | Flashes when interval recording is set.
   [1-CLIP] | Displayed during the one-clip recording mode. [1CLIP] is displayed when a clip can be recorded linked to the previous clip.
   [SIMUL] | Displayed during the simultaneous recording mode. Flashes when the camera cannot record.
   [4G/LTE] | Displayed when connected to 4G/LTE.
   [4G/LTE] | Displayed when not connected to 4G/LTE.
   [4G/LTE] | Displayed when there is an error in the 4G/LTE connection.
   [WLAN] | Displayed when the wireless LAN is operating properly.
   [WLAN] | Displayed when the wireless LAN is not operating properly.
   [LAN] | Displayed when the wired LAN is operating properly.
   [LAN] | Displayed when the wired LAN is not operating properly.
   [PB] | Displayed during the playback mode.
   [OPERATION] | Displayed while operating menus, thumbnails and dialog boxes.

3. Time code indications

   [NDF] | Indicates when the time code is in the non-drop frame mode.
   [DF] | Indicates when the time code is in the drop frame mode.
   [SLAVE] | Indicates when the time code is externally locked.
   [HOLD] | Indicates when the time code generator/read value is held.
   [CTL] | Displayed when <CTL> is selected by the <DISPLAY> switch and the CTL count value is displayed.
   [TCG] | Displayed when <TC> (or <UB>) is selected by the <DISPLAY> switch and the TC (or UB) generator value (h:min:sec:frm) is displayed.
   [TC] | Displayed when <TC> (or <UB>) is selected by the <DISPLAY> switch and the TC (or UB) read value is displayed.
   [VTCG] | Displayed when <UB> is selected by the <DISPLAY> switch and the VIUB generator value is displayed.
   [VTC] | Displayed when <UB> is selected by the <DISPLAY> switch and the VIUB read value is displayed.
   [TIME] | Displayed when <UB> is selected by the <DISPLAY> switch and the real time hours/minutes/seconds value (h:min:sec) is displayed.
   [DATE] | Displayed when <UB> is selected by the <DISPLAY> switch and the real time year/month/day value (Y:M:D) is displayed.
   No display (time zone) | [VTCG], [TIME], and [DATE] are not displayed when <UB> is selected by the <DISPLAY> switch and the real-time hours/minutes value of the time zone is displayed.
   Time counter display | Indicates the time code, user bits, CTL, and real time.

   NOTE

   - When <UB> is selected by the <DISPLAY> switch, each press of the <HOLD> button repeats [VTCG] ([VTC]) → [DATE] → [TIME] → no display (time zone) → [TCG] ([TC]).

4. Mode display

   [W] | Displayed during operation in the SD mode (480/59.94i, 576/50i) and in the 16:9 mode.
   [HD] | Displayed during operation in the HD mode.
   [DV] | Displayed when the recording/playback format is DV.
   [GPS] | Displayed during operation of the built-in GPS. is displayed during GPS communication.
   [eGPS] | Displayed during operation of the external GPS.
   [] (flashing) | Flashes while the camera is being connected to a device which will receive the streaming video.
   [] (illuminated) | Displayed when the camera is connected to a device receiving the streaming video and the camera is transmitting streaming video. The display turns off when a connection could not be established properly.
   [] | Displayed when the rec during upload function is enabled. The display will blink when recording is started immediately after the power is turned on or the P2 card is inserted, and the upload will not be executed until the recording is stopped.
   [] | Displayed during upload.
   [] | Displayed from when transfer error occurred during upload until when the next upload starts.

Top of the page