- Top
- Shooting
- Setting the electronic shutter
- Shutter mode

# Shutter mode

The shutter modes available on the camera’s electronic shutter and shutter speeds that can be selected are as follows.

## Using a fixed shutter speed

- To remove flicker caused by lighting

- To shoot fast-moving subjects clearly

## Using the synchro scan mode

- To shoot so that stripe patterns are eliminated in the horizontal direction when shooting on the monitor screen

- To shoot moving subjects with special effects

## Using the half shutter speed

- To shoot films with special effects

[REC FORMAT] indicates only frame rate. For example, [AVC-I100/60i] is 60i, and [AVC-G50/30PN] is 30P.

[REC FORMAT] | Shutter speed | Half shutter speed | Variable range of synchro scan mode
--- | --- | --- | ---
60P 60i | [1/100], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] | 1/120 | 1/60.1 - 1/7200 | 3.0 deg - 359.5 deg (in 0.5 deg steps)
30P | 1/60 | 1/30.0 - 1/3600
24P | 1/48 | 1/24.0 - 1/2880
50P 50i | [1/60], [1/120], [1/250], [1/500], [1/1000], [1/2000], [HALF], [180.0deg], [172.8deg], [144.0deg], [120.0deg], [90.0deg], [45.0deg] | 1/100 | 1/50.1 - 1/6000
25P | 1/50 | 1/25.0 - 1/3000

Top of the page