- Top
- Shooting
- Viewfinder status display
- Confirmation of return video signal in the viewfinder

# Confirmation of return video signal in the viewfinder

The return video signal input to the <SDI IN> terminal can be viewed in the viewfinder while the <RET> button on the lens is held down. To activate this function, select [CAM RET] in the main menu → [CAMERA] → [SW MODE] → [RET SW].

NOTE

- The HD-Y or VBS signals of the <GENLOCK IN> terminal cannot be viewed as return video signals.

Top of the page