- Top
- Shooting
- Viewfinder status display
- Mode check display

# Mode check display

The camera settings and status can be displayed on the viewfinder screen.

Pushing the <MARKER SEL>/<MODE CHECK/MENU CANCEL> switch on the camera towards the <MCK/MCL> side switches the six screens.

[STATUS] screen display → [!LED] screen display → [FUNCTION] screen display → [AUDIO] screen display → [CAC] screen display → [USER SW STATUS] screen display → no display

Each screen is displayed for approximately five seconds. Pushing the <MARKER SEL>/<MODE CHECK/MENU CANCEL> switch towards the <MCK/MCL> side while the screen is displayed moves the display to the next screen. [ON]/[OFF] of each screen display can be selected in the main menu → [VF] → [MODE CHECK IND]. For details on [STATUS] screen displays, refer to “Checking and displaying shooting status”.

## [!LED] screen

Displays items that are causes of [!LED] lighting.

- [!] is attached to items currently selected at [!LED].

- is attached to items currently targeted for [!LED] lighting.

[GAIN(0dB)] | Displays the gain status.
[DS.GAIN] | Displays the digital super gain value.
[SHUTTER] | Displays the shutter status.
[WHITE PRE.] | Displays the white balance status.
[EXTENDER] | Displays the extender status by [EX]/[OFF].
[B.GAMMA] | Displays the black gamma status by [ON]/[OFF].
[MATRIX] | Displays the [MATRIX] status by [A]/[B]/[OFF].
[COLOR COR.] | Displays the [COLOR CORRECTION] status by [ON]/[OFF].
[FILTER] | Displays the filter status.
[ATW] | Displays the status of automatic tracking white balance.

## [FUNCTION] screen

Displays the video output status and information of the recording media.

[SDI OUT1] | — | Displays the status of the signal output from the <SDI OUT1> terminal.
[OUTPUT] | Displays the status of [MEM]/[CAM] or [OFF] set by [SDI OUT1] and [SDI OUT1 MODE] in the main menu → [I/F SETUP] → [OUTPUT SEL].
[TYPE] | Displays the format of the signal output from the <SDI OUT1> terminal by [HD-SDI]/[SD-SDI].
[CHAR] | Displays the superimposition status of characters selected in the main menu → [I/F SETUP] → [OUTPUT SEL] → [SDI OUT1 CHAR] by [ON]/[OFF].
[SDI OUT2] | — | Displays the status of the signal output from the <SDI OUT2> terminal.
[OUTPUT] | Displays the status of [MEM]/[CAM] or [OFF] set by [SDI OUT2] and [MONITOR OUT MODE] in the main menu → [I/F SETUP] → [OUTPUT SEL].
[SELECT] | Displays the signal format set by [SDI2/HDMI OUT] and [1080P SDI2/HDMI OUT] in the main menu → [I/F SETUP] → [OUTPUT SEL] by [SYSTEM]/[DOWNCON]/[1080i].
[CHAR] | Displays the position of the <MON OUT CHARACTER> switch by [ON]/[OFF].
[P2CARD STATUS] | — | Displays the status of the P2 card inserted in the card slot, remaining capacity and total used capacity. The statuses of cards to be displayed are as follows: [ACTIVE]/[ACCESSING]/[INFO READING]/[FULL]/[PROTECTED]/[NOT SUPPORTED]/[FORMAT ERROR]/[AUTH NG]/[REC IMPOSSIBLE]/[NO CARD] For details, refer to “P2 card access LEDs and status of P2 cards”.
[TOTAL P2/mP2] | Displays the remaining capacity/total capacity totaled for slots 1/2 (or slots 3/4) and the recording medium ([P2] or [mP2]).
[SLOT1] or [SLOT3] | Displays the status of the P2 card in slot 1 (or slot 3) and remaining capacity/total capacity.
[SLOT2] or [SLOT4] | Displays the status of the P2 card in slot 2 (or slot 4) and remaining capacity/total capacity.
[PROXY] | [MEDIA] | Displays the media selection status for proxy recording. [P2]/[P2&SD]/[OFF]
[MODE] | Displays the setting status for proxy recording mode. [STD 2CH MP4]/[SHQ 2CH MOV]/[HQ 4CH MOV]/[HQ 2CH MOV]/[LOW 2CH MOV]/[AVC-G6 2CH]
[SUPER] | Displays the superimposed setting status of the time code. [UPPER]/[LOWER]/[OFF]
[PROXY ERROR] | Displays the operation error on the proxy module.
[NETWORK] | [NETWORK] | Displays the network to be used and its status.

## [AUDIO] screen

Displays audio settings and the selection status of each recording channel.

[SAMPLE RES] | — | Displays the number of audio recording bits.
[MIC POWER (MENU)] | — | Displays the menu setting status of power supply to the microphone.
[FRONT] | Displays the power supply status to the front microphone currently set in the main menu → [I/F SETUP] → [MIC/AUDIO] → [FRONT MIC POWER] by [ON]/[OFF].
[REAR] | Displays whether to set supply of power to the microphone on the <AUDIO IN> terminal at the rear in the main menu → [I/F SETUP] → [MIC/AUDIO] → [REAR MIC POWER]. [OFF]: Power is not supplied to the microphone. [ON]: Power is supplied to the microphone when the <LINE>/<MIC> selector switch is set to <MIC> and the microphone input power selector switch is set to <+48V>.
[VR SELECT] | — | Displays which of [CH1/2] and [CH3/4] the audio level adjustment dial is to be set as enabled to in the main menu → [I/F SETUP] → [MIC/AUDIO] → [VR SELECT].
[LEVEL] | [CH1/2/3/4] | Displays the recording level adjustment method currently selected on each channel. [VR]: Displayed when manual adjustment using the adjustment dial is set. [MENU]: Displayed when manual adjustment using [LVL CONTROL CH3(CH1)]/[LVL CONTROL CH4(CH2)] is set in the main menu → [I/F SETUP] → [MIC/AUDIO]. [AUTO]: Displayed when automatic adjustment is set.
[F.VR] | [CH1/2/3/4] | Displays by [ON]/[OFF] whether the <F.AUDIO LEVEL> dial is enabled on the channel to which [VR] (manual adjustment by adjustment dial) is displayed in [LEVEL].
[A.IN] | [CH1/2/3/4] | Displays the input status of each channel by [FRONT] (front)/[REAR] (rear)/[W.L.] (wireless).
[METER] | [CH1/2/3/4] | Displays the recording level of each channel.

## [CAC INFO] screen

Displays the operation status or information of CAC.

[CAC CONT] | Displays the operation status of CAC. [ON]: [ON] is set to in the main menu → [MAINTENANCE] → [CAC ADJ.] → [CAC CONTROL], and CAC is active. [STOP]: [ON] is set to in the main menu → [MAINTENANCE] → [CAC ADJ.] → [CAC CONTROL], however, CAC operation stops under certain data or lens conditions. [OFF]: [OFF] is set to in the main menu → [MAINTENANCE] → [CAC ADJ.] → [CAC CONTROL], and CAC is not active.
[CAC MODE] | Displays the operation mode of CAC. [AUTO]: The CAC file is automatically selected.
[CONNECT LENS TYPE] | Displays the lens ID of the currently connected digital lens.
[SELECT FILE TITLE] | Displays the title and the file version of the CAC file currently used in the operation. The CAC file can be set in the main menu → [MAINTENANCE] → [CAC ADJ.].
[CAC WARNING] | Displays a warning when operation of CAC has stopped. [CAC LENS DATA INVALID]: This is displayed, for example, when the response data from the lens is not supported. [LENS INIT. NOT COMPLETED]: This is displayed, for example, when initialization of the lens cannot complete.

## [USER SW] screen

Displays the assignment status of each <USER> button. For details, refer to “Assigning functions to <USER> buttons”.

[USER SW] | [USER MAIN (UM)] | Displays the assignment to the <USER MAIN> button.
[USER1 (U1)] | Displays the assignment to the <USER1> button.
[USER2 (U2)] | Displays the assignment to the <USER2> button.
[SHOT MARK (U3)] | Displays the assignment to the <SHOT MARK> button.
[TEXT MEMO (U4)] | Displays the assignment to the <TEXT MEMO> button.
[USER5 (U5)] | Displays the assignment to the <USER5> button.
[OTHER ASSIGN] | [RET SW] | Displays the assignment to the <RET> button on the lens.
[GAIN L] | Displays the gain value assigned to <L> of the <GAIN> switch.
[GAIN M] | Displays the gain value assigned to <M> of the <GAIN> switch.
[GAIN H] | Displays the gain value assigned to <H> of the <GAIN> switch.
[S.GAIN] | Enumerates and displays the gain value assigned as super gain.
[DS.GAIN] | Enumerates and displays the gain value assigned as digital super gain.

Top of the page