- Top
- Network Connection
- Preparing for connection
- For the wireless module AJ-WM30/AJ-WM50

# For the wireless module AJ-WM30/AJ-WM50

Connect the wireless module AJ-WM30/AJ-WM50 (optional) to the camera.

Wireless module fixing part

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Open the cover. (Fig. 1)

Remove the wireless module fixing part from the camera. (Fig. 2)

The wireless module fixing part is secured with a screw.

Securely attach the wireless module to the <USB2.0> terminal (sub-host). (Fig. 3)

(AJ-WM50 only) Place the module holder under the wireless module. (Fig. 4)

- Mount the cap of the wireless module to the hole of the module holder.

Fix the wireless module fixing part removed in step 2 with the screw.

Close the cover.

NOTE

- When removing the wireless module, pull it down straight.

- When using a wireless module other than AJ-WM30/AJ-WM50, refer to “For wireless module other than AJ-WM30/AJ-WM50”.

## Cautions when using wireless module AJ-WM30/AJ-WM50

Read the operating manual of the wireless module thoroughly and understand it before using.

For the latest information, visit the following website:

https://pro-av.panasonic.net/

Top of the page