- Top
- Maintenance
- Warning system
- Error code

# Error code

If errors occur on the camera for any cause, the following error code is displayed on the time code display in the status display. Check the types of warning, and deal with the error according to “Warnings description list”.

Code No. | Message display | Description | Type of warning
--- | --- | --- | ---
First row | Second row
[E-30] | [TURN POWER OFF] | [P2 CARD] | P2 card removal error | Card removal error
[E-31] | [TURN POWER OFF] | [SYSTEM MODE] | System mode error | Mismatched format
[E-33] | [SYSTEM ERROR] | [CAMERA] | Camera unit error | System error
[E-34] | [SYSTEM ERROR] | [LCD MICON] | LCD microcomputer error | System error
[E-35] | [SYSTEM ERROR] | [CODEC] | Codec control error | System error
[E-36] | [SYSTEM ERROR] | [P2 SYSTEM] | P2 system error | System error
[E-37] | [SYSTEM ERROR] | [P2CS] | P2CS microcomputer error | System error
[E-39] | [SYSTEM ERROR] | [INITIALIZE] | Video initialization error | System error
[E-63] | No display | No display | System control microcomputer error | System error
[E-64] | [SYSTEM ERROR] or no display | [FRAME SIGNAL] or no display | Standard signal error | System error

Top of the page