- Top
- Preparation
- Inspections before shooting
- Preparing to inspect

# Preparing to inspect

Fig. 1

Fig. 2

Attach an adequately charged battery.

Set the <POWER> switch to < > (ON) and check the following items.

- [BACKUP BATT EMPTY] is not displayed in the viewfinder screen.

- Level of the battery is sufficient in the status display in the control panel. (Fig. 1)

From the main menu → [REC/PB] → [REC/PB SETUP] → [REC MEDIA], select the P2 card of the recording target slot.

Insert a P2 card into a card slot and close the slot cover. (Fig. 2)

- Ensure that the P2 card access LED lights in orange for the card slot to which the P2 card is inserted. If both card slots have P2 cards inserted, the orange access LED only for the P2 card slot of the P2 card inserted first (the one that completed an access first) lights up, and the green P2 card access LED for the P2 card inserted second lights up.

- If the P2 card access LED for the card slot to which the P2 card is inserted flashes in green or does not light up, that P2 card is not available for recording.

- If the selection of P2 memory card or microP2 memory card does not match the inserted card, the P2 card access LED is not illuminated in orange even when the card is inserted.

  In this case, select the main menu → [REC/PB] → [REC/PB SETUP] → [REC MEDIA], and match the recording target media.

Top of the page