- Top
- Shooting
- Basic procedures
- Standard recording

# Standard recording

Press the <REC> button to start recording of video and audio on the P2 card.

A data consisting of video and sound generated by a single shooting action, together with additional information, is called a “clip”.

<REC> button

NOTE

- In the following cases, it may take time to complete writing to the P2 card.

  Pressing the <REC> button does not accept operations immediately.

  - When short-burst recording is stopped

  - When stopping recording immediately after recording to the second P2 card

- The recording is started using the internal memory of the camera even if the recording is started right after inserting the P2 card is inserted or the power is turned on. In such case, the recording cannot be stopped until the P2 card is recognized. The warning is displayed as [REC PAUSE INVALID] at this time.

  Push the <MARKER SEL>/<MODE CHECK/MENU CANCEL> switch three times towards the <MCK/MCL> side and check the P2 card status on the [SLOT1] and [SLOT2] rows (or, [SLOT3] and [SLOT4]) displayed on the viewfinder screen.

Top of the page