- Top
- Specification
- Details of the connector signals

# Details of the connector signals

DC IN
| 1 | GND
2 | NC
3 | NC
4 | +12 V
Panasonic Parts No.: K1AA104H0038 Manufacturer Parts No.: HA16RX-4P (SW1) (76) (Hirose Electric Co.) NOTE Make sure that the polarity of the external power supply is correct.

FRONT MIC IN
| 1 | GND
2 | L CH IN(H)
3 | L CH IN(C)
4 | R CH IN(H)
5 | R CH IN(C)
Panasonic Parts No.: K1AB105B0002 Manufacturer Parts No.: NC5FBH (NEUTRIK)

AUDIO IN
| 1 | GND
2 | AUDIO IN (H)
3 | AUDIO IN (C)
Panasonic Parts No.: K1AY103A0001 Manufacturer Parts No.: HA16PRM-3SG (72) (Hirose Electric Co.)

AUDIO OUT
| 1 | GND
2 | L CH OUT(H)
3 | L CH OUT(C)
4 | R CH OUT(H)
5 | R CH OUT(C)
Panasonic Parts No.: K1AA105H0016 Manufacturer Parts No.: HA16RD-5P(76) (Hirose Electric Co.) NOTE The <AUDIO OUT> terminal on the camera is the XLR terminal and outputs balanced audio signals. To make unbalanced connection with an external device using a pin plug, release pins 3 and 5. The following is a connection example. Pin terminal Do not use the cable where the pin 3, pin 5 and pin 1 are connected. Doing so may result in a malfunction.

REMOTE
| 1 | CAM DATA (H) | Data from camera to remote control (H)
2 | CAM DATA (C) | Data from camera to remote control (C)
3 | CAM CONT (H) | Control signal from remote control to camera (H)
4 | CAM CONT (C) | Control signal from remote control to camera (C)
5 | R/C ON | Recognition signal of remote control Low: ON
6 | R/C VIDEO OUT | Video signal output to remote control
7 | R/C VIDEO GND | GND for video signal to remote control
8 | NC | Not used
9 | UNREG+12 V | DC 12 V power supply
10 | GND | GND
Panasonic Parts No.: K1AY110JA001 Manufacturer Parts No.: HR10A-10R-10SC (71) (Hirose Electric Co.) Manufacturer Parts No. of cable connector: HR10A-10P-10P(73) (Hirose Electric Co.) NOTE Make sure that the total of the current taken from the <DC OUT> terminal, the <REMOTE> terminal, the <VF> terminal, and the <LENS> terminal does not exceed 2.5 A.

DC OUT
| 1 | GND
2 | R TALLY (open collector)
3 | REC START SW
4 | +12 V OUT DC (11 V – 17 V) (max. 1.5 A)
Panasonic Parts No.: K1AY104J0001 Manufacturer Parts No.: HR10A-7R-4SC (73) (Hirose Electric Co.) Manufacturer Parts No. of cable connector: HR10A-7P-4(73) (Hirose Electric Co.) NOTE Make sure that the total of the current taken from the <DC OUT> terminal, the <REMOTE> terminal, the <VF> terminal, and the <LENS> terminal does not exceed 2.5 A.

VF
| 1 | UNREG-12V | DC 12 V power supply
2 | UNREG-12V | DC 12 V power supply
3 | A9.0V | DC 9 V power supply (not used)
4 | VF-PB-GND | Viewfinder PB signal GND
5 | VF-PR-GND | Viewfinder PR signal GND
6 | VF-Y | Viewfinder Y signal output
7 | VF-Y-GND | Viewfinder Y signal GND
8 | VF-CLK | Serial data clock pulse signal
9 | VF-WR | Pulse signal for serial/parallel conversion data reading
10 | VF-DATA | Serial data signal for serial/parallel conversion
11 | UNREG-GND | GND
12 | ZEBRA-SW | On/off of zebra signal
13 | PEAKING | Peaking control (not used)
14 | SPARE | Spare (not used)
15 | VF-PR | Viewfinder PR signal output
16 | VF-PB | Viewfinder PB signal output
17 | MARKER-SW | Marker ON/OFF (not used)
18 | FRONT-VR | F.AUDIO LEVEL adjustment (not used)
19 | VR-GND | F.AUDIO LEVEL GND (not used)
20 | UNREG-GND | GND
Panasonic Parts No.: K1AB120H0001 Manufacturer Parts No.: HR12-14RA-20SC (Hirose Electric Co.) NOTE Make sure that the total of the current taken from the <DC OUT> terminal, the <REMOTE> terminal, the <VF> terminal, and the <LENS> terminal does not exceed 2.5 A.

LENS
| 1 | RET-SW
2 | REC-START/STOP
3 | GND
4 | IRIS-AUTO
5 | IRIS-CONT
6 | UNREG+12 V (max. 1.5 A)
7 | IRIS-POSI
8 | IRIS-G-MAX
9 | EXT-POSI
10 | ZOOM-POSI
11 | FOCUS-POSI
12 | SPARE
Panasonic Parts No.: K1AY112JA001 Manufacturer Parts No.: HR10A-10R-12SC (71) (Hirose Electric Co.) NOTE Make sure that the total of the current taken from the <DC OUT> terminal, the <REMOTE> terminal, the <VF> terminal, and the <LENS> terminal does not exceed 2.5 A.

Wireless microphone receiver interface
| 1 | CH-1 SHIELD | GND
2 | CH-1 HOT | Audio input from the wireless microphone receiver: CH1 HOT
3 | CH-1 COLD | Audio input from the wireless microphone receiver: CH1 COLD
4 | GND | GND
5 | UNREG +12 V | Power supply to the wireless microphone receiver
6 | RX ON | Power remote output to the wireless microphone receiver
7 | RF WARN | RF warning input from the wireless microphone receiver
8 | RM5 | Not used
9 | RM4 | Not used
10 | SPARE 1 | Not used
11 | SPARE 2 | Not used
12 | EXT CLK | Not used
13 | CLK SHIELD | Not used
14 | CH-2 SHIELD | GND
15 | CH-2 HOT | Audio input from the wireless microphone receiver: CH2 HOT
16 | CH-2 COLD | Audio input from the wireless microphone receiver: CH2 COLD
17 | +5.6 V | Power supply to the wireless microphone receiver
18 | VIDEO OUT | Not used
19 | VIDEO RET | Not used
20 | VIDEO EN | Not used
21 | RM 1 (RM CLK) | Not used
22 | RM 2 (RM DATA) | Not used
23 | RM 3 (RM WR) | Not used
24 | RM+5 V | Not used
25 | RM GND | Not used
Panasonic Parts No.: K1GB25A00010 Manufacturer Parts No.: HDBB-25S (05) (Hirose Electric Co.)

LIGHT
| 1 | 12 V UNREG | Power supply to the light, etc. (supplied from the battery)
2 | GND | GND
Panasonic Parts No.: VJS4444

Top of the page