- Top
- Description of Parts
- Status display
- P2 card, battery charge level, audio level display

# P2 card, battery charge level, audio level display

1. Recording media display

   Displays the recording media.

   [P2] | P2 memory card
   [mP2] | microP2 memory card

2. Media remaining space indicator

   Indicates the remaining free space in the P2 card for each slot using a 7-segment display and remaining time.

   The P2 card remaining time indicated by a single segment is set in three or five minutes in the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [CARD REMAIN/Seg]. Segments go out one segment at a time at each preset time.

   NOTE

   - During loop recording mode, 7 segments up to the [F] position light and are displayed in one line and the time is not displayed.

   - During the simultaneous recording mode, the remaining free space in the P2 card with less space is displayed in one line.

     Indicates the remaining free space in the P2 card for each slot using a 7-segment display and remaining time when either of the media remaining space is low.

3. Battery charge level/power supply voltage display

   The remaining battery charge is displayed by 7 segments and the value of the power supply voltage is displayed. When a battery with a digital indication (% indication) is used, all seven segments up to the [F] position light if the battery charge level is 70% or higher.

   When the battery charge level falls below 70%, the segments go out one by one for each 10% drop. When set [100%] in the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATT REMAIN FULL], seven segments can be set to light at 100%.

4. Audio channel level meter

   When the audio channel selector switch is set to <CH1/2>, audio channel display numbers 1 and 2 are displayed, and the audio level of CH1 and CH2 is displayed. When <CH3/4> is set, audio channel display numbers 3 and 4 are displayed, and the audio level of CH3 and CH4 is displayed.

Top of the page