- Top
- Shooting
- Setting the time data
- How to input user bits

# How to input user bits

By setting user bits, information such as memos (date, time) up to eight digits long (hexadecimal) can be recorded.

1. <DISPLAY> switch

2. Cursor buttons (///)

3. <TCG> switch

Set the <DISPLAY> switch to <UB>.

Set the <TCG> switch to <SET>.

Set the user bits by the cursor buttons.

- Screen display

  - : The digit to be set (flashing) moves to the right.

  - : The digit to be set (flashing) moves to the left.

  - : The value of the digit to set (flashing) is incremented by one.

  - : The value of the digit to set (flashing) is decremented by one.

Set the <TCG> switch to <F-RUN> or <R-RUN>.

Set [USER] in the main menu → [REC/PB] → [TC/UB] → [UBG MODE].

For details, refer to “Setting menu basic operations”.

NOTE

- Thumbnail operations and menu operations on thumbnail operation section are not possible while the <TCG> switch is set to <SET>.

- To confirm VITC UB, press the <HOLD> switch to display [VTCG] on the status display.

## Retention of user bits in memory

User bit settings are automatically recorded and are retained even if the power is turned off.

## Frame rate information recorded on user bits

Saving the frame rate values for the image information shot/saved according to the frame rate set in main menu → [SYSTEM] → [SYSTEM MODE] to user bits allows you to use the editor (personal computer editing software).

Information is always saved in VITC UB.

In addition, selecting [FRAME RATE] in main menu → [REC/PB] → [TC/UB] → [UBG MODE] saves the information in user bits (LTC UB) as well. In playback of clips recorded in native format, the same values as the frame rate information obtained by playing back recorded user bits are also output as HD SDI output signals or user bits of TC output from the <TC OUT> terminal.

### Frame rate information

The relationship between frame rates, image pull-down, and time codes/user bits is as follows.

Media management information

Fixed values

Verification information on the right-hand six digits

Updated frame flags and valid frame flags

REC mark

Sequence No.

24P: 0 - 4

Other than the above: Fixed to F

Camera image mode

Example)

(During shooting)

(VFR 30PN or over 60P)

(VFR over 60P)

(VFR 24PN during shooting)

(VFR 25PN or over 50P)

Top of the page