- Top
- Shooting
- Viewfinder status display
- Lamp display in the viewfinder

# Lamp display in the viewfinder

The example is for the AJ-CVF50G. (For information on the viewfinder, refer to the Operating Instructions for the optional viewfinder.)

1. Green tally lamp

   Lights up green if a green tally signal is received from the Camera Control Unit.

2. TALLY/REC (recording) lamp

   Illuminated red during recording, and flashes if an abnormality occurs.

   For details, refer to “Warning system”.

3. (Irregular operation status warning) lamp

   Lights when the camera enters an irregular operation status among the items set [ON] in the main menu → [VF] → [!LED].

4. BATT (battery) lamp

   Starts flashing when the battery voltage drops and before the battery charge starts to run out. It is illuminated after the battery is completely flat. To prevent operation from being interrupted, replace the battery before it is nearly flat.

   For details, refer to “Warning system”.

5. SAVE lamp

   During regular operation

   - The lamp is out.

   When [SAVE LED] is set to [P2CARD]

   - Flashes when there is little capacity on the P2 card when [P2CARD] is set to in the main menu → [VF] → [VF INDICATOR] → [SAVE LED].

   For details, refer to “Warning system”.

Top of the page