- Top
- Shooting
- Special recording functions
- Recording check function

# Recording check function

- After recording ends, pressing the <RET> button on the lens automatically plays back the last few seconds of the latest clip.

  In this way, you can check whether video has been recorded properly. After playback, the camera is again ready to start recording.

- The recording check function can be assigned to the <USER> buttons (<USER MAIN>/<USER1>/<USER2>). Set [USER MAIN], [USER1], [USER2], [SHOT MARK (U3)], [TEXT MEMO (U4)], or [USER5] to [RET SW] in the main menu → [CAMERA] → [USER SW].

- Holding down the <RET> button for one second plays back from the last ten seconds of the latest clip. During playback at recording check, pressing the <RET> button again stops the playback.

NOTE

- Set [REC CHECK] in main menu → [CAMERA] → [SW MODE] → [RET SW].

- When [SDI OUT1 MODE] or [MONITOR OUT MODE] is set to [MEM] in the main menu → [I/F SETUP] → [OUTPUT SEL], the playback image is output not only to the viewfinder but also the video output terminal (<SDI OUT1> terminal) and the monitor output terminal (<SDI OUT2>, <HDMI OUT> and <VIDEO OUT>) during recording check. Note that when a backup device is connected and the backup image is being recorded, the playback image currently in use by the recording check function will be recorded.

Top of the page