- Top
- Description of Parts
- Audio (input) function section

# Audio (input) function section

1. <F.AUDIO LEVEL> (audio recording level adjustment) dial (Adjustment by <F.AUDIO LEVEL> dial)

   - Adjust the recording level of audio channels 1/2 (or 3/4).

   - Set which of audio channels 1/2 or 3/4 is to be adjusted at the main menu → [I/F SETUP] → [MIC/AUDIO] → [VR SELECT].

   - When the position of the <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> switch is at <AUTO>, adjustment is automatic, and the <F.AUDIO LEVEL> and <AUDIO LEVEL CH1/3>/<AUDIO LEVEL CH2/4> dials do not function.

   - Set whether to enable the <F.AUDIO LEVEL> dial at the main menu → [I/F SETUP] → [MIC/AUDIO] → [FRONT VR CH1(CH3)] or [FRONT VR CH2(CH4)].

2. <AUDIO LEVEL CH1/3>/<AUDIO LEVEL CH2/4> (audio channel 1/3, 2/4 recording level adjustment) dial

   - When the <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> switch is set to <MANU>, the recording level of audio channels 1/2 (3/4) can be adjusted by these dials.

   - Set which of audio channels 1/2 or 3/4 is to be adjusted at the main menu → [I/F SETUP] → [MIC/AUDIO] → [VR SELECT].

   - These knobs have a locking mechanism, so turn the dial while pressing in when making adjustments.

3. <AUDIO IN> (audio input selector) switch

   Select the input signal to be recorded to audio channel 1/2/3/4.

   <FRONT> | Records the microphone input signal connected to the <MIC IN> (microphone input) terminal.
   <W.L.> | Records the input signal from the wireless microphone receiver.
   <REAR> | Records the audio input signal from the audio equipment connected to <AUDIO IN CH1/3> and <AUDIO IN CH2/4> (audio input channels 1/3, 2/4) terminals.

   NOTE

   - When the stereo microphone AJ-MC900G (optional) is used, set both <CH1> and <CH2> (or <CH3> and <CH4>) to <FRONT>. L CH is recorded to <CH1> (<CH3>), and R CH is recorded to <CH2> (<CH4>), respectively.

4. <AUDIO SELECT CH1/3>/<AUDIO SELECT CH2/4> (audio channel 1/3, 2/4/automatic/manual level adjustment selector) switch

   Select the method to adjust the recording level for audio channel 1/2 (3/4).

   <AUTO> | Adjusts automatically.
   <MANU> | Adjusts manually.

   - Set which of audio channels 1/2 or 3/4 is to be adjusted at the main menu → [I/F SETUP] → [MIC/AUDIO] → [VR SELECT].

5. Wireless slot (Using a wireless microphone receiver)

   Mount the UniSlot wireless microphone receiver (optional).

6. <LINE>/<MIC> (line input/microphone input) selector switch (Using audio devices)

   Switch the audio input signal connected to <AUDIO IN CH1/3> and <AUDIO IN CH2/4> (audio input channels 1/3, 2/4) terminals.

   <LINE> | Inputs audio signals from line-input audio equipment.
   <MIC> | Inputs audio signals from the microphone.

7. Microphone input power selector switch (Inspections for using an external microphone)

   Turn on/off the power supply to the microphone connected to the <AUDIO IN CH1/3> and <AUDIO IN CH2/4> (audio input channels 1/3, 2/4) terminals.

   <+48V> | Supplies +48 V power to the microphone.
   <OFF> | Does not supply power to the microphone.

   NOTE

   - When microphone input <+48V> is set and microphones are not connected to the <AUDIO IN CH1/3> and <AUDIO IN CH2/4> terminals, low-frequency noise may occur. This is not a problem when a microphone is connected.

   - When [ON] is not set in the main menu → [I/F SETUP] → [MIC/AUDIO] → [REAR MIC POWER], power is not supplied regardless of the switch position.

8. <AUDIO IN CH1/3>, <AUDIO IN CH2/4> (audio input channel 1/3, 2/4) terminals (Using audio devices)

   Connect the audio equipment or the microphone.

9. <MIC IN> (microphone input) terminal (Preparing for audio input)

   - Connect the microphone (optional).

   - The phantom microphone can also be used. To use this, set [ON] in the main menu → [I/F SETUP] → [MIC/AUDIO] → [FRONT MIC POWER]. When it is set to [ON] and a microphone is not connected, low-frequency noise may occur. This is not a problem when a microphone is connected.

Top of the page