- Top
- Connecting to External Devices
- Connecting to Remote operation panel (AK-HRP200G)

# Connecting to Remote operation panel (AK-HRP200G)

You can remote control some functions by connecting the remote operation panel AK-HRP200G (optional) to the camera's <LAN> terminal or <REMOTE> terminal.

It is necessary to set AK-HRP200G with the ROP setup software included in AK-HRP200G for the IP connection between AK-HRP200G and the <LAN> terminal of the camera, or for the serial connection with the <REMOTE> terminal of the camera.

For detailed setting procedure, refer to the Operating Instructions of AK-HRP200G.

#### When connecting to the camera's <LAN> terminal

- When you connect AK-HRP200G via wired LAN and perform network settings of the camera and the AK-HRP200G, the camera automatically enters the remote control mode. For the settings of connection, refer to “Setting for IP connection with the remote operation panel (AK-HRP200G)”.

- The remote control mode is canceled by pressing the <HEAD POWER> switch of AK-HRP200G to terminate the connection while the camera and AK-HRP200G are connected, or by removing the network cable and changing the <POWER> switch from < > (standby) to < > (ON).

LAN cable (optional)

AK-HRP200G

#### When connecting to the camera's <REMOTE> terminal

- The camera will automatically go into the remote control mode when the serial connection is made between AK-HRP200G in which the serial connection setting has been made and the camera, and the <POWER> switch of the camera is set to < > (ON).

- The remote control mode is canceled with following methods.

  - Disconnect the cable connecting the camera with AK-HRP200G.

  - Terminate the connection by pressing the <HEAD POWER> switch of AK-HRP200G while it is still connected.

<REMOTE> terminal

AK-HRP200G

Switch functionality in remote control mode
Recording and playback operations in remote control mode
Remote control unit connected to the camera

NOTE

- To use the camera as a standalone device, the remote control mode must be disabled.

- The operation of connecting via IP and remote controlling the camera from multiple devices such as the AK-HRP200G cannot be guaranteed.

- For details, refer to the Operating Instructions of AK-HRP200G.

- When the camera is connected to AK-HRP200G via IP, the P2 playlist editing function is not available.

Top of the page