- Top
- Menu Operations
- Menu list
- [FILE]

# [FILE]

These are items for performing file-related operations such as reading from an SD memory card containing menu settings data, and handling lens files and lens chromatic aberration correction (CAC) files.

These menu items cannot be set when the thumbnail screen is displayed or during playback.

[FILE] menu cannot be operated in the following cases:

- While the thumbnail screen is displayed

  Remedy: Press the <THUMBNAIL> button to close the thumbnail screen, and try the operations again.

- During playback

  Remedy: Press the <STOP> button to stop playback, and try the operations again.

- When recording by linking to the previous clip is possible in one-clip recording mode (when [1CLIP] is displayed at the bottom right in the viewfinder and the LCD monitor)

  Remedy: Close the menu once, and hold down the <STOP> button for approx. 2 seconds to end linking of clips, and then try the operation again.

- During standby in interval recording or one-shot recording

  Remedy: Press the <STOP> button to end interval recording, and try the operation again.

## [SETUP DATA (SD CARD)]

Item | Description of settings
--- | ---
[LOAD] | Loads the file selected from the setup data file list saved to the SD memory card to the camera. The data selected in [SETUP DATA SELECT] is loaded.
[SAVE] | Overwrites the current menu setting values in the camera to the file selected from the existing file list saved to the SD memory card. Data selected in [SETUP DATA SELECT] is saved.
[SAVE AS] | Enters the current menu setting values of the camera to file name and title as a new file and saves it to the SD memory card. Data selected in [SETUP DATA SELECT] is saved.

## [SETUP DATA SELECT]

- Select menu items to save to/read from to SD memory card in the main menu → [FILE] → [SETUP DATA (SD CARD)].

- The factory settings are as follows:

  - [SYSTEM], [CAMERA ID], [OPTION MENU] → without [✓]

  - Other → [✓] present

Item | Description of settings
--- | ---
[SYSTEM] | Handles the menu in the main menu → [SYSTEM].
[CAMERA ID] | Handles the menu in the main menu → [CAMERA] → [CAMERA ID].
[USER MENU SEL] | Handles the menu in the main menu → [USER MENU SEL].
[PAINT(LEVEL)] | Handles the menu adjustment value in the main menu → [PAINT].
[PAINT([S]SELECT)] | Handles the menu setting value (items with [S]) in the main menu → [PAINT].
[VF] | Handles the menu in the main menu → [VF].
[CAMERA] | Handles the menu in the main menu → [CAMERA].
[REC/PB] | Handles the menu in the main menu → [REC/PB].
[CLIP] | Handles the menu setting value in the main menu → [CLIP].
[I/F SETUP] | Handles the menu in the main menu → [I/F SETUP].
[MAINTENANCE] | Handles the menu setting value in the main menu → [MAINTENANCE].
[OPTION MENU] | Handles [OPTION MENU].

## [CAC FILE (SD CARD)]

Item | Description of settings
--- | ---
[LOAD] | Selects the chromatic aberration compensation data file saved to the SD memory card and loads to the camera. Specifies the file number when saving chromatic aberration compensation data of the SD memory card loaded in [LOAD] to the camera.
[DELETE] | Selects and deletes the chromatic aberration compensation data file saved to the SD memory card.

## [LENS FILE]

Item | Description of settings
--- | ---
[LOAD] | Selects the lens file saved to the camera memory, loads it and uses it as a setting value for the current operation.
[SAVE] | Specifies and saves the title and number of current lens setting values to the memory of this camera.
[CLEAR ALL FILE] | Clears and initializes all values saved to the lens file.

## [LENS FILE (SD CARD)]

Item | Description of settings
--- | ---
[LOAD] | Selects a lens file saved to the SD memory card and loads it as one set of lens files (8 file set) in the camera.
[SAVE] | Specifies and saves the title and number of a lens file (1set of 8 files) in the camera to the SD memory card.

## [SCENE]

Item | Description of settings
--- | ---
[LOAD] | Selects and loads a scene file saved in the camera memory.
[SAVE] | Specifies a title and file number for the current setting values and saves them as a scene file in the camera memory.
[CLEAR] | Selects and initializes a scene file saved in the camera memory. The title is removed and saved data is returned to factory settings.

## [SD CARD PROPERTY]

Displays the SD memory card status.

The format condition, available space, etc. can be confirmed.

Item | Description of settings
--- | ---
[SD STANDARD] | Indicates whether an SD memory card is formatted according to the SD/SDHC/SDXC standard. [SUPPORTED]: Complies with SD/SDHC/SDXC standards [NOT SUPPORTED]: Does not comply with SD/SDHC/SDXC standards
[USED] | Displays used capacity (bytes).
[BLANK] | Displays available space (bytes).
[TOTAL] | Displays total capacity (bytes).
[PROXY REM] | Displays remaining recording capacity of SD card when recording proxy.
[NUMBER OF CLIPS] | Copy and proxy records display the clip quantity inside an SD memory card.
[PROTECT] | Write prohibited.

## [FORMAT SD CARD]

Formats an SD memory card.

## [LOAD USER DATA]

Loads a user file saved in the camera memory.

## [INITIALIZE]

Item | Description of settings
--- | ---
[LOAD FACTORY DATA] | All menu values are set to factory settings. The following data is not returned to factory settings. Scene files User data Lens files Black shading data
[SAVE USER DATA] | User menu setting values are saved as user data in the camera memory. Can be used as saved data the user can uniquely set. Load user data in the main menu → [FILE] → [LOAD USER DATA].

Top of the page