- Top
- Preparation
- Power supply
- Mounting and setting battery

# Mounting and setting battery

## Using Anton/Bauer batteries

Release lever

Anton/Bauer batteries

Mount the Anton/Bauer battery.

Insert the battery terminal and slide in the direction of the arrow.

Set the battery type.

Select the battery in the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT].

For details, refer to “Setting menu basic operations”.

NOTE

- To remove the battery, keep the release lever of the battery holder completely down, slide the battery in the opposite direction of when you mounted it.

## Using V-mount type batteries

Mount the V-mount type battery plate. As shown in the figure, insert and slide in the direction of the arrow.

Release lever

Mount the V-mount type battery plate.

Slide in the direction of the arrow.

Set the battery type.

- Select the battery type in the main menu → [I/F SETUP] → [BATTERY/P2CARD] → [BATTERY SELECT].

NOTE

- Contact your dealer for information about the V-mount type battery plate.

- When the V-mount type battery plate is used, % (percent) is not displayed even if batteries with a battery level indicator function are used.

- When removing the plate, remove by sliding the release lever.

- When using a battery that is not in the [BATTERY SELECT] item, set [TYPE A], [TYPE B] or [TYPE C], and set each item according to the characteristics of the battery.

  For details, refer to [BATTERY/P2CARD] and [BATTERY SETTING].

Top of the page