- Top
- Network Connection
- Network connection

# Network connection

The camera can be connected to the network via wireless LAN, wired LAN, or 4G/LTE.

Also, high speed network connection is possible when connected to the bonding device to wireless LAN or wired LAN.

To use wireless LAN, attach AJ-WM30/AJ-WM50 (optional) to the <USB2.0> terminal (sub-host).

For details on wireless module and bonding device that can be connected, refer to the support desk at the following website.

https://pro-av.panasonic.net/

To use wired LAN, connect a LAN cable to the <LAN> terminal on the rear side.

To use 4G/LTE, connect a 4G/LTE USB modem that is compliant with the <USB2.0> terminal (sub-host).

IEEE802.11g/n

100BASE-TX/10BASE-T

Available functions
Operating environment
Top of the page